(footprint "LOOPY_EdgeConnector_Socket" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr through_hole)
  (fp_text reference "J**" (at 0 -8.6) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 06747bd5-23a7-484c-b80b-aab481b0130a)
  )
  (fp_text value "Loopy_EdgeConnector_Socket" (at 0 7.6) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 3d5d3a33-edd5-4e62-bf91-f30c978a840c)
  )
  (fp_line (start -58 -7) (end -60 -5)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp d0493910-f95e-4b68-8c07-63d9c521a5b2))
  (fp_line (start 60 -5) (end 58 -7)
    (stroke (width 0.12) (type default)) (layer "F.SilkS") (tstamp 667cca78-ba94-49f2-8abd-aa4b53b60091))
  (fp_rect (start -60 -7) (end 60 7)
    (stroke (width 0.12) (type default)) (fill none) (layer "F.SilkS") (tstamp 26e6c6a8-0208-4cbd-a8e5-0f9bfb466100))
  (fp_poly
    (pts
      (xy 1.5 9)
      (xy 0 10)
      (xy -1.5 9)
    )

    (stroke (width 0.12) (type solid)) (fill solid) (layer "F.SilkS") (tstamp 155fa70a-7069-4363-90ad-182333d0d782))
  (fp_rect (start -60 -7) (end 60 7)
    (stroke (width 0.05) (type default)) (fill none) (layer "F.CrtYd") (tstamp 697d51d1-9277-46fa-b991-20c1fe4b01c9))
  (pad "" np_thru_hole oval (at -55.2 0) (size 8 8) (drill 7) (layers "*.Mask")
    (thermal_bridge_angle 45) (tstamp 7295b284-2a88-4792-a006-02157a96e498))
  (pad "" np_thru_hole oval (at -49.2 0) (size 2 2) (drill 2) (layers "*.Mask")
    (thermal_bridge_angle 45) (tstamp 57569eb1-5b76-414d-880b-e97a1fcfdd10))
  (pad "" np_thru_hole oval (at 49.2 0) (size 2 2) (drill 2) (layers "*.Mask")
    (thermal_bridge_angle 45) (tstamp aed6a0fa-535b-4604-814e-e0c031cabd40))
  (pad "" np_thru_hole oval (at 55.2 -0.1) (size 8 8) (drill 7) (layers "*.Mask")
    (thermal_bridge_angle 45) (tstamp b5eae423-3ff4-4866-bcfc-bf34ba9955a7))
  (pad "1" thru_hole oval (at 46.2 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp aa10eb9b-d366-4d52-a534-b5315c368793))
  (pad "2" thru_hole oval (at 44.1 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 1b3bad92-5af6-4e9f-853e-cb7a0ca1947a))
  (pad "3" thru_hole oval (at 42 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 6df0be84-f5e4-4f6b-be3a-954bcad4ae4a))
  (pad "4" thru_hole oval (at 39.9 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 4f9f639a-61d3-4e59-9a17-74ca72b5b3b9))
  (pad "5" thru_hole oval (at 37.8 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 3dfb43db-209d-4cb9-bb31-0e0f7cb2842e))
  (pad "6" thru_hole oval (at 35.7 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp ae17926d-42ce-4d8e-b233-209d3868174f))
  (pad "7" thru_hole oval (at 33.6 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 5b18f7bb-bfc8-4ffb-8623-b29337433ee1))
  (pad "8" thru_hole oval (at 31.5 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 3d7fb091-3fa9-4a6f-b3c8-7ef69086fed5))
  (pad "9" thru_hole oval (at 29.4 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 8ae46e2d-1f34-4dd2-9b40-194bf4dc81aa))
  (pad "10" thru_hole oval (at 27.3 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp eb880ead-e22d-4112-86b0-bdf824f8ae5d))
  (pad "11" thru_hole oval (at 25.2 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp b917b215-e271-45eb-8653-09dcb16e35ad))
  (pad "12" thru_hole oval (at 23.1 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 2e563899-d446-4358-b1cb-e361c6dc36d5))
  (pad "13" thru_hole oval (at 21 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 07c8f2b7-e19a-4a9e-b75c-bbfd269f4aa9))
  (pad "14" thru_hole oval (at 18.9 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 48874278-b2c7-4dab-a504-7523177d6ff8))
  (pad "15" thru_hole oval (at 16.8 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 01706190-00d1-48ca-9f4a-cfb592bdf2f9))
  (pad "16" thru_hole oval (at 14.7 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 8a5faade-8640-4953-a14c-2f3daf87ace9))
  (pad "17" thru_hole oval (at 12.6 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 6e7b0881-aa43-4b9f-af00-987841615b50))
  (pad "18" thru_hole oval (at 10.5 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp e6efbc4f-c7cc-43fa-99c7-59fc1f97db6a))
  (pad "19" thru_hole oval (at 8.4 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 388d31bd-efa6-4078-ad82-0e06c64e458a))
  (pad "20" thru_hole oval (at 6.3 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 1e2aa138-31b5-40ac-8021-6e97d9074c0a))
  (pad "21" thru_hole oval (at 4.2 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 93d533b7-b81e-4526-a228-116bf461ddf4))
  (pad "22" thru_hole oval (at 2.1 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp cfcb304e-0d0c-4b2b-8d91-d8a649c487ac))
  (pad "23" thru_hole oval (at 0 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp d2f3e0f3-08ea-4ae2-b16d-c3c28c58f1c2))
  (pad "24" thru_hole oval (at -2.1 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 13b5a3a0-9f2a-4bdf-a1f7-66f874b76536))
  (pad "25" thru_hole oval (at -4.2 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 15bfac56-5f05-4080-9b2e-a190d08544c4))
  (pad "26" thru_hole oval (at -6.3 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 3b107ef4-0dea-4fec-9aa9-1c4805e649e3))
  (pad "27" thru_hole oval (at -8.4 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 81651b0d-46c1-4c2c-8601-c490d0d36886))
  (pad "28" thru_hole oval (at -10.5 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp c677846c-168f-442a-a938-38e6f109e68d))
  (pad "29" thru_hole oval (at -12.6 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp d5154dd2-45f3-42da-80d1-483d14eaa303))
  (pad "30" thru_hole oval (at -14.7 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 62181ab5-a808-47a3-a7a6-8350c3b3e003))
  (pad "31" thru_hole oval (at -16.8 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 21d5ffe3-c615-4d55-9830-f1104d1a9dd2))
  (pad "32" thru_hole oval (at -18.9 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 19cff9b1-5e8b-4f38-afe4-7d65a7a991c7))
  (pad "33" thru_hole oval (at -21 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 6e1de706-b2e5-46eb-a5e1-8bcc901d0c73))
  (pad "34" thru_hole oval (at -23.1 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 8221f393-3ecc-473a-a2e2-164f93b190c7))
  (pad "35" thru_hole oval (at -25.2 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 5a0d2aa2-c42e-48a4-bd26-be3163c90810))
  (pad "36" thru_hole oval (at -27.3 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 2b00e973-02a2-41da-b79b-a3fa711bebfd))
  (pad "37" thru_hole oval (at -29.4 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 6e613806-f21c-416b-b94b-7ed37aa36202))
  (pad "38" thru_hole oval (at -31.5 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 7cf81623-2de7-4659-9b67-d592b8150462))
  (pad "39" thru_hole oval (at -33.6 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 195d8e7c-ab13-48e3-8e79-3081789167bc))
  (pad "40" thru_hole oval (at -35.7 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 0aeb4f1f-da25-44e1-ada7-0db1749dc380))
  (pad "41" thru_hole oval (at -37.8 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp abc64090-c147-4c6e-98e5-69521e47028b))
  (pad "42" thru_hole oval (at -39.9 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 2ba6c534-22ca-40c4-b44f-210887a48a6d))
  (pad "43" thru_hole oval (at -42 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 415e0d8b-67a3-47a4-b420-3243c1100419))
  (pad "44" thru_hole oval (at -44.1 -4.7) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 3f7e0c66-189d-46fe-8546-c0d867278991))
  (pad "45" thru_hole oval (at -46.2 -1.55) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 75cf1d10-30de-490a-8ec9-7e9a8405148c))
  (pad "46" thru_hole oval (at 46.2 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp d2559797-4f35-4281-ab49-dfd31a3cee16))
  (pad "47" thru_hole oval (at 44.1 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 7b18ffe2-97a8-4ff5-9ea5-20034be47876))
  (pad "48" thru_hole oval (at 42 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 0dbddf36-7943-4f62-88ee-4ed8a9b5e7ac))
  (pad "49" thru_hole oval (at 39.9 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 636937d6-a57d-4f5b-9e4e-9e4033a35cf3))
  (pad "50" thru_hole oval (at 37.8 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp a83468fa-7485-44bb-9228-fb68fdce4119))
  (pad "51" thru_hole oval (at 35.7 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 41f59134-82a5-41d6-acf2-b8b885bf874d))
  (pad "52" thru_hole oval (at 33.6 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp fb2d4f48-fb10-4a25-8765-d8ace61e2ca0))
  (pad "53" thru_hole oval (at 31.5 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 1e3e038c-fd0f-4036-aa93-596ce5514e4a))
  (pad "54" thru_hole oval (at 29.4 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 453fb365-7796-4e27-91d8-9ec4dcc962e5))
  (pad "55" thru_hole oval (at 27.3 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp d25faacc-d530-4096-bce3-99793c9aed16))
  (pad "56" thru_hole oval (at 25.2 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 7d82d0b4-b398-4907-ac73-2286b73527aa))
  (pad "57" thru_hole oval (at 23.1 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp f2c597d8-9a24-4016-a721-09fac46980d2))
  (pad "58" thru_hole oval (at 21 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp ed96ae2a-a801-4a12-9177-f98e8bf64474))
  (pad "59" thru_hole oval (at 18.9 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp b499d3a1-c891-4510-b5b5-7608705483d7))
  (pad "60" thru_hole oval (at 16.8 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp dc4dc85c-6575-46ce-88dd-cbf50629f951))
  (pad "61" thru_hole oval (at 14.7 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 2f9e83bb-d1b5-40bb-bdff-b9b9d0e511b7))
  (pad "62" thru_hole oval (at 12.6 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp a11b520f-fbc5-4d1f-a86c-2e4f4d24ab78))
  (pad "63" thru_hole oval (at 10.5 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp d9adb757-b8d8-49e7-b2e1-cdc244d84a3e))
  (pad "64" thru_hole oval (at 8.4 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 4ad5f771-a21c-46fd-b41f-a099bdae32a8))
  (pad "65" thru_hole oval (at 6.3 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 2f6caf21-e7bd-41de-ad62-ff67f08a73d0))
  (pad "66" thru_hole oval (at 4.2 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 1cbee837-a872-4130-b958-9d9f779f4b99))
  (pad "67" thru_hole oval (at 2.1 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp d8d6ada6-8787-4467-bcc9-aad9efb8f5e8))
  (pad "68" thru_hole oval (at 0 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp f96ab9c9-0ae2-4a18-95c0-30f4c433b09d))
  (pad "69" thru_hole oval (at -2.1 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp d37f5e87-157a-45fe-9430-b6e9a85db6f5))
  (pad "70" thru_hole oval (at -4.2 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp a8b2686a-5afc-4b4c-9732-d6c0ebeea1df))
  (pad "71" thru_hole oval (at -6.3 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 89ab5ff1-5cc3-435b-a8f5-bb6af9d26d49))
  (pad "72" thru_hole oval (at -8.4 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp e5bd67ff-8300-460a-86de-d534823a8aa3))
  (pad "73" thru_hole oval (at -10.5 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 2ac10ef0-9b99-4a7b-91d1-1e791db39e2b))
  (pad "74" thru_hole oval (at -12.6 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 8ee369b9-9b2a-4856-b251-eb5751ac8007))
  (pad "75" thru_hole oval (at -14.7 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp fe34214a-6699-4d22-8507-616c9618a71c))
  (pad "76" thru_hole oval (at -16.8 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp f8fcfff7-f03d-4469-847f-098619953c47))
  (pad "77" thru_hole oval (at -18.9 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp b2645d57-cd50-440f-b3eb-f6b2e0c22613))
  (pad "78" thru_hole oval (at -21 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 8cf5fddd-090d-4106-b9d8-23d9d691e55e))
  (pad "79" thru_hole oval (at -23.1 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp e8a57044-d2eb-4335-8eb7-37d21c10b373))
  (pad "80" thru_hole oval (at -25.2 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp fe1114c8-6d98-4179-9d36-7454db88d6a5))
  (pad "81" thru_hole oval (at -27.3 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp dc664e9e-efb7-49a4-b0c9-e05861835c59))
  (pad "82" thru_hole oval (at -29.4 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 0d67b35a-6b90-4cd0-b30d-719c89a0abea))
  (pad "83" thru_hole oval (at -31.5 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 69ba89ee-c3a4-4317-a04b-24ea8de7f44c))
  (pad "84" thru_hole oval (at -33.6 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 20b3ac4c-2146-4111-bc00-9adfa0a94f21))
  (pad "85" thru_hole oval (at -35.7 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp a7c35e0b-9958-4da1-9700-d7d170b95987))
  (pad "86" thru_hole oval (at -37.8 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp c6920759-5697-4c85-a4e5-ac6bdbd16d38))
  (pad "87" thru_hole oval (at -39.9 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 3f4be141-939e-4a8d-a11f-bb82e61cc707))
  (pad "88" thru_hole oval (at -42 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp 95545e69-03f3-4255-a5ec-0c50f640fc9e))
  (pad "89" thru_hole oval (at -44.1 1.6) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp cc8d2c41-8c3a-452e-b006-b78eaf4061d2))
  (pad "90" thru_hole oval (at -46.2 4.75) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
    (thermal_bridge_angle 45) (tstamp d79ae947-417c-4d5e-8be6-3f7d93397a7e))
)
