(kicad_symbol_lib (version 20220914) (generator kicad_symbol_editor)
  (symbol "FC_Slot" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -16.51 52.07 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "FC_Slot" (at -13.97 46.99 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "!OSCR:FC_Slot" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "FC_Slot_0_1"
      (rectangle (start -17.78 44.45) (end 17.78 -34.29)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
    )
    (symbol "FC_Slot_1_1"
      (pin power_in line (at -20.32 41.91 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 19.05 0) (length 2.54)
        (name "PRG_A3" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 16.51 0) (length 2.54)
        (name "PRG_A2" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 13.97 0) (length 2.54)
        (name "PRG_A1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 11.43 0) (length 2.54)
        (name "PRG_A0" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 8.89 0) (length 2.54)
        (name "PRG_RW" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 6.35 0) (length 2.54)
        (name "IRQ" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -20.32 3.81 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 1.27 0) (length 2.54)
        (name "CHR_RD" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 -1.27 0) (length 2.54)
        (name "CIRAM_A10" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 -3.81 0) (length 2.54)
        (name "CHR_A6" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 39.37 0) (length 2.54)
        (name "PRG_A11" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 -6.35 0) (length 2.54)
        (name "CHR_A5" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 -8.89 0) (length 2.54)
        (name "CHR_A4" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 -11.43 0) (length 2.54)
        (name "CHR_A3" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 -13.97 0) (length 2.54)
        (name "CHR_A2" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 -16.51 0) (length 2.54)
        (name "CHR_A1" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 -19.05 0) (length 2.54)
        (name "CHR_A0" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -21.59 0) (length 2.54)
        (name "CHR_D0" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -24.13 0) (length 2.54)
        (name "CHR_D1" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -26.67 0) (length 2.54)
        (name "CHR_D2" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -29.21 0) (length 2.54)
        (name "CHR_D3" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 36.83 0) (length 2.54)
        (name "PRG_A10" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -20.32 -31.75 0) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 20.32 41.91 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 39.37 180) (length 2.54)
        (name "M2" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 36.83 180) (length 2.54)
        (name "PRG_A12" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 34.29 180) (length 2.54)
        (name "PRG_A13" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 31.75 180) (length 2.54)
        (name "PRG_A14" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 29.21 180) (length 2.54)
        (name "PRG_D7" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 26.67 180) (length 2.54)
        (name "PRG_D6" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 24.13 180) (length 2.54)
        (name "PRG_D5" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 21.59 180) (length 2.54)
        (name "PRG_D4" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 34.29 0) (length 2.54)
        (name "PRG_A9" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 19.05 180) (length 2.54)
        (name "PRG_D3" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 16.51 180) (length 2.54)
        (name "PRG_D2" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 13.97 180) (length 2.54)
        (name "PRG_D1" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 11.43 180) (length 2.54)
        (name "PRG_D0" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 8.89 180) (length 2.54)
        (name "PRG_CE" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 20.32 6.35 180) (length 2.54)
        (name "EXP" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 20.32 3.81 180) (length 2.54)
        (name "EXP" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 1.27 180) (length 2.54)
        (name "CHR_WR" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 -1.27 180) (length 2.54)
        (name "CIRAM_CE" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 -3.81 180) (length 2.54)
        (name "CHR_/A13" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 31.75 0) (length 2.54)
        (name "PRG_A8" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -6.35 180) (length 2.54)
        (name "CHR_A7" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 -8.89 180) (length 2.54)
        (name "CHR_A8" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 -11.43 180) (length 2.54)
        (name "CHR_A9" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 -13.97 180) (length 2.54)
        (name "CHR_A10" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 -16.51 180) (length 2.54)
        (name "CHR_A11" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 -19.05 180) (length 2.54)
        (name "CHR_A12" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 20.32 -21.59 180) (length 2.54)
        (name "CHR_A13" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -24.13 180) (length 2.54)
        (name "CHR_D7" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -26.67 180) (length 2.54)
        (name "CHR_D6" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -29.21 180) (length 2.54)
        (name "CHR_D5" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 29.21 0) (length 2.54)
        (name "PRG_A7" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -31.75 180) (length 2.54)
        (name "CHR_D4" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 26.67 0) (length 2.54)
        (name "PRG_A6" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 24.13 0) (length 2.54)
        (name "PRG_A5" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -20.32 21.59 0) (length 2.54)
        (name "PRG_A4" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "GBA_Slot" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at -39.37 15.24 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "GBA_Slot" (at -35.56 11.43 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "!OSCR:GBA_Slot" (at -19.05 15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -19.05 15.24 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "GBA_Slot_0_0"
      (pin power_in line (at 40.64 -8.89 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "SH1" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 40.64 -8.89 90) (length 2.54) hide
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "SH2" (effects (font (size 1.27 1.27))))
      )
    )
    (symbol "GBA_Slot_0_1"
      (rectangle (start 41.91 -6.35) (end -39.37 10.16)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
    )
    (symbol "GBA_Slot_1_1"
      (pin power_in line (at -38.1 -8.89 90) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -8.89 90) (length 2.54)
        (name "AD4" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -8.89 90) (length 2.54)
        (name "AD5" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -8.89 90) (length 2.54)
        (name "AD6" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -7.62 -8.89 90) (length 2.54)
        (name "AD7" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -5.08 -8.89 90) (length 2.54)
        (name "AD8" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -2.54 -8.89 90) (length 2.54)
        (name "AD9" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 0 -8.89 90) (length 2.54)
        (name "AD10" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 2.54 -8.89 90) (length 2.54)
        (name "AD11" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 5.08 -8.89 90) (length 2.54)
        (name "AD12" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 7.62 -8.89 90) (length 2.54)
        (name "AD13" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -35.56 -8.89 90) (length 2.54)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 10.16 -8.89 90) (length 2.54)
        (name "AD14" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -8.89 90) (length 2.54)
        (name "AD15" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 15.24 -8.89 90) (length 2.54)
        (name "D0_A16" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -8.89 90) (length 2.54)
        (name "D1_A17" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 20.32 -8.89 90) (length 2.54)
        (name "D2_A18" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -8.89 90) (length 2.54)
        (name "D3_A19" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 25.4 -8.89 90) (length 2.54)
        (name "D4_A20" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 27.94 -8.89 90) (length 2.54)
        (name "D5_A21" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 30.48 -8.89 90) (length 2.54)
        (name "D6_A22" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 33.02 -8.89 90) (length 2.54)
        (name "D7_A23" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -33.02 -8.89 90) (length 2.54)
        (name "WR" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 35.56 -8.89 90) (length 2.54)
        (name "RST_CS2" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 38.1 -8.89 90) (length 2.54)
        (name "AUD_IRQ" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 40.64 -8.89 90) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -30.48 -8.89 90) (length 2.54)
        (name "RD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -27.94 -8.89 90) (length 2.54)
        (name "CS1" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -25.4 -8.89 90) (length 2.54)
        (name "AD0" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -22.86 -8.89 90) (length 2.54)
        (name "AD1" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -20.32 -8.89 90) (length 2.54)
        (name "AD2" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -17.78 -8.89 90) (length 2.54)
        (name "AD3" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "Loopy_Slot" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 0 1.27 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "Loopy_Slot" (at 0 0 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "Loopy_Slot_1_1"
      (rectangle (start -7.62 0) (end 7.62 -116.84)
        (stroke (width 0) (type default))
        (fill (type background))
      )
      (pin power_in line (at -11.43 -2.54 0) (length 3.81)
        (name "+5V" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -11.43 -25.4 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -11.43 -27.94 0) (length 3.81)
        (name "~{RAMWE}" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -11.43 -30.48 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -11.43 -33.02 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -11.43 -35.56 0) (length 3.81)
        (name "+5V" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -38.1 0) (length 3.81)
        (name "PA15" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -40.64 0) (length 3.81)
        (name "PB1" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -43.18 0) (length 3.81)
        (name "PB9" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -45.72 0) (length 3.81)
        (name "PB10" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -48.26 0) (length 3.81)
        (name "PB11" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -5.08 0) (length 3.81)
        (name "AR" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -50.8 0) (length 3.81)
        (name "PB8" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -53.34 0) (length 3.81)
        (name "PB12" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -55.88 0) (length 3.81)
        (name "A12" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -58.42 0) (length 3.81)
        (name "A10" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -60.96 0) (length 3.81)
        (name "A8" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -63.5 0) (length 3.81)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -66.04 0) (length 3.81)
        (name "A13" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -68.58 0) (length 3.81)
        (name "A15" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -71.12 0) (length 3.81)
        (name "A20" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin power_out line (at -11.43 -73.66 0) (length 3.81)
        (name "+5V" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -7.62 0) (length 3.81)
        (name "AVCC" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -76.2 0) (length 3.81)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -78.74 0) (length 3.81)
        (name "A21" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -81.28 0) (length 3.81)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -83.82 0) (length 3.81)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -11.43 -86.36 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -88.9 0) (length 3.81)
        (name "D0" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -11.43 -91.44 0) (length 3.81)
        (name "~{RESET}" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -93.98 0) (length 3.81)
        (name "D2" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -96.52 0) (length 3.81)
        (name "D3" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -99.06 0) (length 3.81)
        (name "D14" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -10.16 0) (length 3.81)
        (name "AL" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -101.6 0) (length 3.81)
        (name "D4" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -104.14 0) (length 3.81)
        (name "D6" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -106.68 0) (length 3.81)
        (name "D8" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -11.43 -109.22 0) (length 3.81)
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -11.43 -111.76 0) (length 3.81)
        (name "D10" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -11.43 -114.3 0) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 11.43 -114.3 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 11.43 -111.76 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 11.43 -109.22 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -106.68 180) (length 3.81)
        (name "AGND" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -11.43 -12.7 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -104.14 180) (length 3.81)
        (name "VSYNC" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -101.6 180) (length 3.81)
        (name "VFB" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 11.43 -99.06 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -96.52 180) (length 3.81)
        (name "RH_P56" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 11.43 -93.98 180) (length 3.81)
        (name "~{CS6}" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 11.43 -91.44 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -88.9 180) (length 3.81)
        (name "~{OE}" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 11.43 -86.36 180) (length 3.81)
        (name "+5V" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 11.43 -83.82 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 11.43 -81.28 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -11.43 -15.24 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -78.74 180) (length 3.81)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -76.2 180) (length 3.81)
        (name "PB3" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -73.66 180) (length 3.81)
        (name "PB5" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -71.12 180) (length 3.81)
        (name "PB7" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -68.58 180) (length 3.81)
        (name "PB13" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -66.04 180) (length 3.81)
        (name "PB14" (effects (font (size 1.27 1.27))))
        (number "65" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at 11.43 -63.5 180) (length 3.81)
        (name "PB15" (effects (font (size 1.27 1.27))))
        (number "66" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -60.96 180) (length 3.81)
        (name "A11" (effects (font (size 1.27 1.27))))
        (number "67" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -58.42 180) (length 3.81)
        (name "A9" (effects (font (size 1.27 1.27))))
        (number "68" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -55.88 180) (length 3.81)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "69" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -11.43 -17.78 0) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -53.34 180) (length 3.81)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "70" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -50.8 180) (length 3.81)
        (name "A14" (effects (font (size 1.27 1.27))))
        (number "71" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -48.26 180) (length 3.81)
        (name "A17" (effects (font (size 1.27 1.27))))
        (number "72" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -45.72 180) (length 3.81)
        (name "A16" (effects (font (size 1.27 1.27))))
        (number "73" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -43.18 180) (length 3.81)
        (name "A18" (effects (font (size 1.27 1.27))))
        (number "74" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 11.43 -40.64 180) (length 3.81)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "75" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -38.1 180) (length 3.81)
        (name "A19" (effects (font (size 1.27 1.27))))
        (number "76" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -35.56 180) (length 3.81)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "77" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -33.02 180) (length 3.81)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "78" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 11.43 -30.48 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "79" (effects (font (size 1.27 1.27))))
      )
      (pin passive line (at -11.43 -20.32 0) (length 3.81)
        (name "CVID" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 11.43 -27.94 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "80" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -25.4 180) (length 3.81)
        (name "D1" (effects (font (size 1.27 1.27))))
        (number "81" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -22.86 180) (length 3.81)
        (name "D12" (effects (font (size 1.27 1.27))))
        (number "82" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -20.32 180) (length 3.81)
        (name "D13" (effects (font (size 1.27 1.27))))
        (number "83" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -17.78 180) (length 3.81)
        (name "D15" (effects (font (size 1.27 1.27))))
        (number "84" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -15.24 180) (length 3.81)
        (name "D5" (effects (font (size 1.27 1.27))))
        (number "85" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -12.7 180) (length 3.81)
        (name "D7" (effects (font (size 1.27 1.27))))
        (number "86" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 11.43 -10.16 180) (length 3.81)
        (name "" (effects (font (size 1.27 1.27))))
        (number "87" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -7.62 180) (length 3.81)
        (name "D9" (effects (font (size 1.27 1.27))))
        (number "88" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 11.43 -5.08 180) (length 3.81)
        (name "+5V" (effects (font (size 1.27 1.27))))
        (number "89" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -11.43 -22.86 0) (length 3.81)
        (name "~{CS2}" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 11.43 -2.54 180) (length 3.81)
        (name "D11" (effects (font (size 1.27 1.27))))
        (number "90" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "MD_Slot" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -1.27 39.37 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "MD_Slot" (at 1.27 36.83 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "!OSCR:MD_Slot" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "MD_Slot_0_1"
      (rectangle (start -7.62 20.32) (end 20.32 -63.5)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
    )
    (symbol "MD_Slot_1_1"
      (pin power_in line (at 22.86 17.78 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "A1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 -5.08 180) (length 2.54)
        (name "A14" (effects (font (size 1.27 1.27))))
        (number "A10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 -7.62 180) (length 2.54)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "A11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 -10.16 180) (length 2.54)
        (name "A15" (effects (font (size 1.27 1.27))))
        (number "A12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 -12.7 180) (length 2.54)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "A13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 -15.24 180) (length 2.54)
        (name "A16" (effects (font (size 1.27 1.27))))
        (number "A14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 -17.78 180) (length 2.54)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "A15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 -20.32 180) (length 2.54)
        (name "A17" (effects (font (size 1.27 1.27))))
        (number "A16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 -22.86 180) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "A17" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -25.4 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "A18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -27.94 180) (length 2.54)
        (name "D7" (effects (font (size 1.27 1.27))))
        (number "A19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 15.24 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "A2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -30.48 180) (length 2.54)
        (name "D0" (effects (font (size 1.27 1.27))))
        (number "A20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -33.02 180) (length 2.54)
        (name "D8" (effects (font (size 1.27 1.27))))
        (number "A21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -35.56 180) (length 2.54)
        (name "D6" (effects (font (size 1.27 1.27))))
        (number "A22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -38.1 180) (length 2.54)
        (name "D1" (effects (font (size 1.27 1.27))))
        (number "A23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -40.64 180) (length 2.54)
        (name "D9" (effects (font (size 1.27 1.27))))
        (number "A24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -43.18 180) (length 2.54)
        (name "D5" (effects (font (size 1.27 1.27))))
        (number "A25" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -45.72 180) (length 2.54)
        (name "D2" (effects (font (size 1.27 1.27))))
        (number "A26" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -48.26 180) (length 2.54)
        (name "D10" (effects (font (size 1.27 1.27))))
        (number "A27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -50.8 180) (length 2.54)
        (name "D4" (effects (font (size 1.27 1.27))))
        (number "A28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -53.34 180) (length 2.54)
        (name "D3" (effects (font (size 1.27 1.27))))
        (number "A29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 12.7 180) (length 2.54)
        (name "A8" (effects (font (size 1.27 1.27))))
        (number "A3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 22.86 -55.88 180) (length 2.54)
        (name "D11" (effects (font (size 1.27 1.27))))
        (number "A30" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -58.42 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "A31" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 22.86 -60.96 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "A32" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 10.16 180) (length 2.54)
        (name "A11" (effects (font (size 1.27 1.27))))
        (number "A4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 7.62 180) (length 2.54)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "A5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 5.08 180) (length 2.54)
        (name "A12" (effects (font (size 1.27 1.27))))
        (number "A6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 2.54 180) (length 2.54)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "A7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 0 180) (length 2.54)
        (name "A13" (effects (font (size 1.27 1.27))))
        (number "A8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 22.86 -2.54 180) (length 2.54)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "A9" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 17.78 0) (length 2.54)
        (name "SL1" (effects (font (size 1.27 1.27))))
        (number "B1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -5.08 0) (length 2.54)
        (name "A22" (effects (font (size 1.27 1.27))))
        (number "B10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -7.62 0) (length 2.54)
        (name "A23" (effects (font (size 1.27 1.27))))
        (number "B11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -10.16 0) (length 2.54)
        (name "/YS" (effects (font (size 1.27 1.27))))
        (number "B12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -12.7 0) (length 2.54)
        (name "/VSYNC" (effects (font (size 1.27 1.27))))
        (number "B13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -15.24 0) (length 2.54)
        (name "/HSYNC" (effects (font (size 1.27 1.27))))
        (number "B14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -17.78 0) (length 2.54)
        (name "EDCLK" (effects (font (size 1.27 1.27))))
        (number "B15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -20.32 0) (length 2.54)
        (name "/CAS0" (effects (font (size 1.27 1.27))))
        (number "B16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -22.86 0) (length 2.54)
        (name "/CE_0" (effects (font (size 1.27 1.27))))
        (number "B17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -25.4 0) (length 2.54)
        (name "/AS" (effects (font (size 1.27 1.27))))
        (number "B18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -27.94 0) (length 2.54)
        (name "VCLK" (effects (font (size 1.27 1.27))))
        (number "B19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 15.24 0) (length 2.54)
        (name "/MRES" (effects (font (size 1.27 1.27))))
        (number "B2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -30.48 0) (length 2.54)
        (name "/DTACK" (effects (font (size 1.27 1.27))))
        (number "B20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -33.02 0) (length 2.54)
        (name "/CAS2" (effects (font (size 1.27 1.27))))
        (number "B21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -35.56 0) (length 2.54)
        (name "D15" (effects (font (size 1.27 1.27))))
        (number "B22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -38.1 0) (length 2.54)
        (name "D14" (effects (font (size 1.27 1.27))))
        (number "B23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -40.64 0) (length 2.54)
        (name "D13" (effects (font (size 1.27 1.27))))
        (number "B24" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -10.16 -43.18 0) (length 2.54)
        (name "D12" (effects (font (size 1.27 1.27))))
        (number "B25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -45.72 0) (length 2.54)
        (name "/ASEL" (effects (font (size 1.27 1.27))))
        (number "B26" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -48.26 0) (length 2.54)
        (name "/VRES" (effects (font (size 1.27 1.27))))
        (number "B27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -50.8 0) (length 2.54)
        (name "/LWR" (effects (font (size 1.27 1.27))))
        (number "B28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -53.34 0) (length 2.54)
        (name "/UWR" (effects (font (size 1.27 1.27))))
        (number "B29" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -10.16 12.7 0) (length 2.54)
        (name "SR1" (effects (font (size 1.27 1.27))))
        (number "B3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -55.88 0) (length 2.54)
        (name "/M3" (effects (font (size 1.27 1.27))))
        (number "B30" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -58.42 0) (length 2.54)
        (name "/TIME" (effects (font (size 1.27 1.27))))
        (number "B31" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -60.96 0) (length 2.54)
        (name "/CART" (effects (font (size 1.27 1.27))))
        (number "B32" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 10.16 0) (length 2.54)
        (name "A9" (effects (font (size 1.27 1.27))))
        (number "B4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 7.62 0) (length 2.54)
        (name "A10" (effects (font (size 1.27 1.27))))
        (number "B5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 5.08 0) (length 2.54)
        (name "A18" (effects (font (size 1.27 1.27))))
        (number "B6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 2.54 0) (length 2.54)
        (name "A19" (effects (font (size 1.27 1.27))))
        (number "B7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 0 0) (length 2.54)
        (name "A20" (effects (font (size 1.27 1.27))))
        (number "B8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -10.16 -2.54 0) (length 2.54)
        (name "A21" (effects (font (size 1.27 1.27))))
        (number "B9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "N64_Slot" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at -10.16 35.56 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "N64_Slot" (at -6.35 33.02 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "!OSCR:N64 Slot" (at -5.08 20.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -5.08 20.32 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "N64_Slot_0_1"
      (rectangle (start -10.16 31.75) (end 15.24 -34.29)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
    )
    (symbol "N64_Slot_1_1"
      (pin power_in line (at -12.7 29.21 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 6.35 0) (length 2.54)
        (name "/READ" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 3.81 0) (length 2.54)
        (name "AD11" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 1.27 0) (length 2.54)
        (name "AD10" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 -1.27 0) (length 2.54)
        (name "12V" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -12.7 -3.81 0) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -6.35 0) (length 2.54)
        (name "AD9" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -8.89 0) (length 2.54)
        (name "AD8" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 -11.43 0) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -12.7 -13.97 0) (length 2.54)
        (name "CIC_to_PIF" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -16.51 0) (length 2.54)
        (name "EEPROM_CLK" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 26.67 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 -19.05 0) (length 2.54)
        (name "RESET" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 -21.59 0) (length 2.54)
        (name "EEPROM_DATA" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 -24.13 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 -26.67 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -12.7 -29.21 0) (length 2.54)
        (name "L_AUDIO" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 -31.75 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 29.21 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 26.67 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 24.13 180) (length 2.54)
        (name "AD0" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 21.59 180) (length 2.54)
        (name "AD1" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 24.13 0) (length 2.54)
        (name "AD15" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 19.05 180) (length 2.54)
        (name "AD2" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 16.51 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 13.97 180) (length 2.54)
        (name "AD3" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 17.78 11.43 180) (length 2.54)
        (name "ALE_L" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 8.89 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 17.78 6.35 180) (length 2.54)
        (name "ALE_H" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 3.81 180) (length 2.54)
        (name "AD4" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 1.27 180) (length 2.54)
        (name "AD5" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -1.27 180) (length 2.54)
        (name "12V" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 17.78 -3.81 180) (length 2.54)
        (name "NC" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 21.59 0) (length 2.54)
        (name "AD14" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -6.35 180) (length 2.54)
        (name "AD6" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 17.78 -8.89 180) (length 2.54)
        (name "AD7" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -11.43 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 17.78 -13.97 180) (length 2.54)
        (name "PIF_to_CIC" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 17.78 -16.51 180) (length 2.54)
        (name "R4300_CLK" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 17.78 -19.05 180) (length 2.54)
        (name "NMI" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 17.78 -21.59 180) (length 2.54)
        (name "Video_CLK" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -24.13 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -26.67 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 17.78 -29.21 180) (length 2.54)
        (name "R_Audio" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 19.05 0) (length 2.54)
        (name "AD13" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 17.78 -31.75 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 16.51 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -12.7 13.97 0) (length 2.54)
        (name "AD12" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -12.7 11.43 0) (length 2.54)
        (name "/WRITE" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -12.7 8.89 0) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "NES_Slot" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -16.51 44.45 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "NES_Slot" (at -12.7 41.91 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "!OSCR:NES_Slot" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "NES_Slot_0_1"
      (rectangle (start -16.51 39.37) (end 19.05 -54.61)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
    )
    (symbol "NES_Slot_1_1"
      (pin power_in line (at -19.05 -52.07 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -29.21 0) (length 2.54)
        (name "PRG_A3" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -26.67 0) (length 2.54)
        (name "PRG_A2" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -24.13 0) (length 2.54)
        (name "PRG_A1" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -21.59 0) (length 2.54)
        (name "PRG_A0" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -19.05 0) (length 2.54)
        (name "PRG_RW" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -16.51 0) (length 2.54)
        (name "IRQ" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -19.05 -13.97 0) (length 2.54)
        (name "EXP_0" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -19.05 -11.43 0) (length 2.54)
        (name "EXP_1" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -19.05 -8.89 0) (length 2.54)
        (name "EXP_2" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -19.05 -6.35 0) (length 2.54)
        (name "EXP_3" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -49.53 0) (length 2.54)
        (name "PRG_A11" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -19.05 -3.81 0) (length 2.54)
        (name "EXP_4" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -1.27 0) (length 2.54)
        (name "CHR_RD" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 1.27 0) (length 2.54)
        (name "CIRAM_A10" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 3.81 0) (length 2.54)
        (name "CHR_A6" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 6.35 0) (length 2.54)
        (name "CHR_A5" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 8.89 0) (length 2.54)
        (name "CHR_A4" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 11.43 0) (length 2.54)
        (name "CHR_A3" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 13.97 0) (length 2.54)
        (name "CHR_A2" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 16.51 0) (length 2.54)
        (name "CHR_A1" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 19.05 0) (length 2.54)
        (name "CHR_A0" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -46.99 0) (length 2.54)
        (name "PRG_A10" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -19.05 21.59 0) (length 2.54)
        (name "CHR_D0" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -19.05 24.13 0) (length 2.54)
        (name "CHR_D1" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -19.05 26.67 0) (length 2.54)
        (name "CHR_D2" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -19.05 29.21 0) (length 2.54)
        (name "CHR_D3" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -19.05 31.75 0) (length 2.54)
        (name "Security3" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at -19.05 34.29 0) (length 2.54)
        (name "Security4" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -19.05 36.83 0) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -52.07 180) (length 2.54)
        (name "CLK" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -49.53 180) (length 2.54)
        (name "M2" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -46.99 180) (length 2.54)
        (name "PRG_A12" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -44.45 0) (length 2.54)
        (name "PRG_A9" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -44.45 180) (length 2.54)
        (name "PRG_A13" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -41.91 180) (length 2.54)
        (name "PRG_A14" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 -39.37 180) (length 2.54)
        (name "PRG_D7" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 -36.83 180) (length 2.54)
        (name "PRG_D6" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 -34.29 180) (length 2.54)
        (name "PRG_D5" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 -31.75 180) (length 2.54)
        (name "PRG_D4" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 -29.21 180) (length 2.54)
        (name "PRG_D3" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 -26.67 180) (length 2.54)
        (name "PRG_D2" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 -24.13 180) (length 2.54)
        (name "PRG_D1" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 -21.59 180) (length 2.54)
        (name "PRG_D0" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -41.91 0) (length 2.54)
        (name "PRG_A8" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -19.05 180) (length 2.54)
        (name "PRG_CE" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 21.59 -16.51 180) (length 2.54)
        (name "EXP_9" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 21.59 -13.97 180) (length 2.54)
        (name "EXP_8" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 21.59 -11.43 180) (length 2.54)
        (name "EXP_7" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 21.59 -8.89 180) (length 2.54)
        (name "EXP_6" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 21.59 -6.35 180) (length 2.54)
        (name "EXP_5" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -3.81 180) (length 2.54)
        (name "CHR_WR" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -1.27 180) (length 2.54)
        (name "CIRAM_CE" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 1.27 180) (length 2.54)
        (name "CHR_/A13" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 3.81 180) (length 2.54)
        (name "CHR_A7" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -39.37 0) (length 2.54)
        (name "PRG_A7" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 6.35 180) (length 2.54)
        (name "CHR_A8" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 8.89 180) (length 2.54)
        (name "CHR_A9" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 11.43 180) (length 2.54)
        (name "CHR_A11" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 13.97 180) (length 2.54)
        (name "CHR_A10" (effects (font (size 1.27 1.27))))
        (number "63" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 16.51 180) (length 2.54)
        (name "CHR_A12" (effects (font (size 1.27 1.27))))
        (number "64" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 19.05 180) (length 2.54)
        (name "CHR_A13" (effects (font (size 1.27 1.27))))
        (number "65" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 21.59 180) (length 2.54)
        (name "CHR_D7" (effects (font (size 1.27 1.27))))
        (number "66" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 24.13 180) (length 2.54)
        (name "CHR_D6" (effects (font (size 1.27 1.27))))
        (number "67" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 26.67 180) (length 2.54)
        (name "CHR_D5" (effects (font (size 1.27 1.27))))
        (number "68" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 29.21 180) (length 2.54)
        (name "CHR_D4" (effects (font (size 1.27 1.27))))
        (number "69" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -36.83 0) (length 2.54)
        (name "PRG_A6" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 21.59 31.75 180) (length 2.54)
        (name "Security1" (effects (font (size 1.27 1.27))))
        (number "70" (effects (font (size 1.27 1.27))))
      )
      (pin no_connect line (at 21.59 34.29 180) (length 2.54)
        (name "Security2" (effects (font (size 1.27 1.27))))
        (number "71" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 21.59 36.83 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "72" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -34.29 0) (length 2.54)
        (name "PRG_A5" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -31.75 0) (length 2.54)
        (name "PRG_A4" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SMS_Slot" (in_bom yes) (on_board yes)
    (property "Reference" "U" (at -10.16 35.56 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SMS_Slot" (at -6.35 33.02 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "!OSCR:SMS_Slot" (at -6.35 33.02 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at -6.35 33.02 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SMS_Slot_0_1"
      (rectangle (start -11.43 30.48) (end 10.16 -35.56)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
    )
    (symbol "SMS_Slot_1_1"
      (pin power_in line (at 12.7 -33.02 180) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 -22.86 0) (length 2.54)
        (name "A11" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -20.32 180) (length 2.54)
        (name "M0-7" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 -20.32 0) (length 2.54)
        (name "A10" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -17.78 180) (length 2.54)
        (name "CE" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -13.97 -17.78 0) (length 2.54)
        (name "D7" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -15.24 180) (length 2.54)
        (name "D6" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -13.97 -15.24 0) (length 2.54)
        (name "D5" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -12.7 180) (length 2.54)
        (name "D4" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -13.97 -12.7 0) (length 2.54)
        (name "D3" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.7 -10.16 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 -33.02 0) (length 2.54)
        (name "WR" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -13.97 -10.16 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.7 -7.62 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -13.97 -7.62 0) (length 2.54)
        (name "D2" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 12.7 -5.08 180) (length 2.54)
        (name "D1" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -13.97 -5.08 0) (length 2.54)
        (name "D0" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -2.54 180) (length 2.54)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 -2.54 0) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 0 180) (length 2.54)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 0 0) (length 2.54)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 2.54 180) (length 2.54)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -30.48 180) (length 2.54)
        (name "MReq" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 2.54 0) (length 2.54)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 5.08 180) (length 2.54)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 5.08 0) (length 2.54)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 7.62 180) (length 2.54)
        (name "A12" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 7.62 0) (length 2.54)
        (name "CONT" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 12.7 10.16 180) (length 2.54)
        (name "5V" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 10.16 0) (length 2.54)
        (name "A15" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 12.7 180) (length 2.54)
        (name "M1" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 12.7 0) (length 2.54)
        (name "IOReq" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 15.24 180) (length 2.54)
        (name "Refresh" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 -30.48 0) (length 2.54)
        (name "RD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 15.24 0) (length 2.54)
        (name "Halt" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 17.78 180) (length 2.54)
        (name "Wait" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 17.78 0) (length 2.54)
        (name "Int" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 20.32 180) (length 2.54)
        (name "JyDs" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 20.32 0) (length 2.54)
        (name "BusReq" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 22.86 180) (length 2.54)
        (name "BusAck" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 22.86 0) (length 2.54)
        (name "Reset" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 25.4 180) (length 2.54)
        (name "Clock" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 25.4 0) (length 2.54)
        (name "JRead" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 27.94 180) (length 2.54)
        (name "MC-F" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -27.94 180) (length 2.54)
        (name "M8-B" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 27.94 0) (length 2.54)
        (name "NMI" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 -27.94 0) (length 2.54)
        (name "A14" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -25.4 180) (length 2.54)
        (name "A13" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -13.97 -25.4 0) (length 2.54)
        (name "A8" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 -22.86 180) (length 2.54)
        (name "A9" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "SNES_Slot" (in_bom yes) (on_board yes)
    (property "Reference" "J" (at 12.7 45.72 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "SNES_Slot" (at -11.43 45.72 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "!OSCR:SNES Slot" (at 0 44.45 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (at 0 44.45 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "SNES_Slot_0_1"
      (rectangle (start -16.51 44.45) (end 19.05 -46.99)
        (stroke (width 0.1524) (type default))
        (fill (type none))
      )
    )
    (symbol "SNES_Slot_1_1"
      (pin input line (at -19.05 41.91 0) (length 2.54)
        (name "21.477MHz_Clock" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 13.97 0) (length 2.54)
        (name "A7" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 11.43 0) (length 2.54)
        (name "A6" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 8.89 0) (length 2.54)
        (name "A5" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 6.35 0) (length 2.54)
        (name "A4" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 3.81 0) (length 2.54)
        (name "A3" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 1.27 0) (length 2.54)
        (name "A2" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -1.27 0) (length 2.54)
        (name "A1" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -3.81 0) (length 2.54)
        (name "A0" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -6.35 0) (length 2.54)
        (name "/IRQ" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -19.05 -8.89 0) (length 2.54)
        (name "D0" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 39.37 0) (length 2.54)
        (name "Expand" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -19.05 -11.43 0) (length 2.54)
        (name "D1" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -19.05 -13.97 0) (length 2.54)
        (name "D2" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -19.05 -16.51 0) (length 2.54)
        (name "D3" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -19.05 0) (length 2.54)
        (name "/RD" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -19.05 -21.59 0) (length 2.54)
        (name "CIC_out_data_(p1)" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -24.13 0) (length 2.54)
        (name "CIC_in_data_(p7)" (effects (font (size 1.27 1.27))))
        (number "25" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -26.67 0) (length 2.54)
        (name "/RESET" (effects (font (size 1.27 1.27))))
        (number "26" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -19.05 -29.21 0) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "27" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -36.83 0) (length 2.54)
        (name "PA0" (effects (font (size 1.27 1.27))))
        (number "28" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -39.37 0) (length 2.54)
        (name "PA2" (effects (font (size 1.27 1.27))))
        (number "29" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 36.83 0) (length 2.54)
        (name "PA6" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -41.91 0) (length 2.54)
        (name "PA4" (effects (font (size 1.27 1.27))))
        (number "30" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 -44.45 0) (length 2.54)
        (name "Left_Audio_Input" (effects (font (size 1.27 1.27))))
        (number "31" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 41.91 180) (length 2.54)
        (name "/WRAM" (effects (font (size 1.27 1.27))))
        (number "32" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 39.37 180) (length 2.54)
        (name "Refresh" (effects (font (size 1.27 1.27))))
        (number "33" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 36.83 180) (length 2.54)
        (name "PA7" (effects (font (size 1.27 1.27))))
        (number "34" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 34.29 180) (length 2.54)
        (name "/PAWR" (effects (font (size 1.27 1.27))))
        (number "35" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 21.59 26.67 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "36" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 24.13 180) (length 2.54)
        (name "A12" (effects (font (size 1.27 1.27))))
        (number "37" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 21.59 180) (length 2.54)
        (name "A13" (effects (font (size 1.27 1.27))))
        (number "38" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 19.05 180) (length 2.54)
        (name "A14" (effects (font (size 1.27 1.27))))
        (number "39" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 34.29 0) (length 2.54)
        (name "/PARD" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 16.51 180) (length 2.54)
        (name "A15" (effects (font (size 1.27 1.27))))
        (number "40" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 13.97 180) (length 2.54)
        (name "BA0" (effects (font (size 1.27 1.27))))
        (number "41" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 11.43 180) (length 2.54)
        (name "BA1" (effects (font (size 1.27 1.27))))
        (number "42" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 8.89 180) (length 2.54)
        (name "BA2" (effects (font (size 1.27 1.27))))
        (number "43" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 6.35 180) (length 2.54)
        (name "BA3" (effects (font (size 1.27 1.27))))
        (number "44" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 3.81 180) (length 2.54)
        (name "BA4" (effects (font (size 1.27 1.27))))
        (number "45" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 1.27 180) (length 2.54)
        (name "BA5" (effects (font (size 1.27 1.27))))
        (number "46" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -1.27 180) (length 2.54)
        (name "BA6" (effects (font (size 1.27 1.27))))
        (number "47" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -3.81 180) (length 2.54)
        (name "BA7" (effects (font (size 1.27 1.27))))
        (number "48" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -6.35 180) (length 2.54)
        (name "/Cart" (effects (font (size 1.27 1.27))))
        (number "49" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at -19.05 26.67 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 -8.89 180) (length 2.54)
        (name "D4" (effects (font (size 1.27 1.27))))
        (number "50" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 -11.43 180) (length 2.54)
        (name "D5" (effects (font (size 1.27 1.27))))
        (number "51" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 -13.97 180) (length 2.54)
        (name "D6" (effects (font (size 1.27 1.27))))
        (number "52" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 21.59 -16.51 180) (length 2.54)
        (name "D7" (effects (font (size 1.27 1.27))))
        (number "53" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -19.05 180) (length 2.54)
        (name "/WR" (effects (font (size 1.27 1.27))))
        (number "54" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 21.59 -21.59 180) (length 2.54)
        (name "CIC_data_out_(p2)" (effects (font (size 1.27 1.27))))
        (number "55" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -24.13 180) (length 2.54)
        (name "CIC_clock_in_(p6)" (effects (font (size 1.27 1.27))))
        (number "56" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -26.67 180) (length 2.54)
        (name "CPU_Clock" (effects (font (size 1.27 1.27))))
        (number "57" (effects (font (size 1.27 1.27))))
      )
      (pin power_in line (at 21.59 -29.21 180) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "58" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -36.83 180) (length 2.54)
        (name "PA1" (effects (font (size 1.27 1.27))))
        (number "59" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 24.13 0) (length 2.54)
        (name "A11" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -39.37 180) (length 2.54)
        (name "PA3" (effects (font (size 1.27 1.27))))
        (number "60" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -41.91 180) (length 2.54)
        (name "PA5" (effects (font (size 1.27 1.27))))
        (number "61" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 21.59 -44.45 180) (length 2.54)
        (name "Right_Audio_Input" (effects (font (size 1.27 1.27))))
        (number "62" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 21.59 0) (length 2.54)
        (name "A10" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 19.05 0) (length 2.54)
        (name "A9" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -19.05 16.51 0) (length 2.54)
        (name "A8" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
