(footprint "GBA_Slot" (version 20211014) (generator pcbnew) (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "U$4" (at 0 0) (layer "F.SilkS") hide
    (effects (font (size 1.27 1.27) (thickness 0.15)))
    (tstamp 315d130f-fb4a-4e2d-922c-9e6bfbb047d6)
  )
  (fp_text value "GBA_Slot" (at 0 0) (layer "F.SilkS") hide
    (effects (font (size 1.27 1.27) (thickness 0.15)))
    (tstamp b4e0ed8a-f6a5-4975-b653-8752d6c2ed32)
  )
  (fp_text user "1" (at -1.79 -23.68 270) (layer "F.SilkS")
    (effects (font (size 1.2065 1.2065) (thickness 0.1016)) (justify left bottom))
    (tstamp 7fbd67a2-ff82-4932-89ca-8556fa396a71)
  )
  (fp_line (start 15 -28) (end 15 -25.5) (layer "F.Fab") (width 0.1) (tstamp 034bb61a-0d29-4e7c-afd9-40d06727f107))
  (fp_line (start -2.5 25.5) (end -2.5 28) (layer "F.Fab") (width 0.1) (tstamp 06b34d7d-829a-46d4-b2b9-2ee2203f9ef4))
  (fp_line (start 15 -25.5) (end 15 25.5) (layer "F.Fab") (width 0.1) (tstamp 39069e01-d43d-4744-8388-124ea9097729))
  (fp_line (start 15 28) (end 15 28.5) (layer "F.Fab") (width 0.1) (tstamp 5791502b-3a9d-4d7e-a3f3-f230c2303546))
  (fp_line (start -2.5 -28.5) (end -2.5 -28) (layer "F.Fab") (width 0.1) (tstamp 81707840-0e01-47ec-8c89-f2aeac35b613))
  (fp_line (start 15 28) (end 15 25.5) (layer "F.Fab") (width 0.1) (tstamp 8c230e53-9b09-48fd-b94d-32e25be321c6))
  (fp_line (start 15 -28.5) (end -2.5 -28.5) (layer "F.Fab") (width 0.1) (tstamp 902164e7-4b7a-4c51-b9a1-76afedc7de55))
  (fp_line (start -2.5 -25.5) (end -4 -25.5) (layer "F.Fab") (width 0.1) (tstamp 9d1f4ba8-e8ef-4e50-a857-0b7d4155ef67))
  (fp_line (start -2.5 -25.5) (end -2.5 -28) (layer "F.Fab") (width 0.1) (tstamp 9ebce03f-647d-47f4-b598-acb0fe9a5b38))
  (fp_line (start -4 25.5) (end -2.5 25.5) (layer "F.Fab") (width 0.1) (tstamp a1367cac-94d4-472e-a7e7-8c6e98c2c7c2))
  (fp_line (start 15 -28) (end 15 -28.5) (layer "F.Fab") (width 0.1) (tstamp b317a772-d54a-4547-a810-5b114abdfd99))
  (fp_line (start 15 28.5) (end -2.5 28.5) (layer "F.Fab") (width 0.1) (tstamp bf289ccb-760b-4740-b215-36e02d5366ba))
  (fp_line (start -2.5 28) (end -2.5 28.5) (layer "F.Fab") (width 0.1) (tstamp e6e44424-fa19-4082-9018-94749cdfd6f4))
  (fp_line (start -4 -25.5) (end -4 25.5) (layer "F.Fab") (width 0.1) (tstamp e8e3a367-94c6-4bd0-bd02-008f19a9cc32))
  (pad "" np_thru_hole circle locked (at 3.5 13) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask) (tstamp 966ae2d2-6cfa-4e77-b99e-e7d5ce70df84))
  (pad "" np_thru_hole circle locked (at 3.5 -13) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask) (tstamp a82f76f0-a28b-4751-a907-24573ac6f04a))
  (pad "1" smd rect locked (at -5 -23.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp b23a0f63-d965-40b0-bc39-c7fefa62e97c))
  (pad "2" smd rect locked (at -5 -21.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp dedc4871-4cf9-464f-9cef-a3ee6a4e4416))
  (pad "3" smd rect locked (at -5 -20.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 8d96c569-9d79-4c13-bf6b-aab072b7c9b4))
  (pad "4" smd rect locked (at -5 -18.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 4eeb9df1-efaf-4175-8586-46b04ca33919))
  (pad "5" smd rect locked (at -5 -17.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 5ebe21c5-461e-41d9-b971-58894f4c10ec))
  (pad "6" smd rect locked (at -5 -15.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp b57d7ef6-3e3b-46b2-88bc-9599e7d0dab8))
  (pad "7" smd rect locked (at -5 -14.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 40d294cd-ac8f-46e4-9849-11cb62957601))
  (pad "8" smd rect locked (at -5 -12.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp e39f4d15-dc16-4c3f-bb70-e6377b786186))
  (pad "9" smd rect locked (at -5 -11.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 83389a3b-00e2-4b34-bac4-b447dfd24b35))
  (pad "10" smd rect locked (at -5 -9.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp d7fc1da8-2bd0-48c6-a8b4-3007630e3f1e))
  (pad "11" smd rect locked (at -5 -8.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 209faede-471e-4992-a354-8960898440a6))
  (pad "12" smd rect locked (at -5 -6.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 357f0c08-fc6d-49a0-b2e2-4632d3654173))
  (pad "13" smd rect locked (at -5 -5.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp ce747902-a204-46e1-bf23-e081f3d7e14f))
  (pad "14" smd rect locked (at -5 -3.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 99338b9d-6514-47d7-b338-05461cb0cc5a))
  (pad "15" smd rect locked (at -5 -2.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 90cec09f-4e40-4581-8bca-1e2838155e2b))
  (pad "16" smd rect locked (at -5 -0.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 25aab775-f6f0-49c1-8e5f-5a6807d93b99))
  (pad "17" smd rect locked (at -5 0.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp de55583f-97b6-4da2-9477-a8f9a25ea4c8))
  (pad "18" smd rect locked (at -5 2.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp e7742b2e-af48-4204-aa25-3b1fc6f55cb5))
  (pad "19" smd rect locked (at -5 3.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 507e291e-e2e4-49c0-8349-bb0c2c21eb22))
  (pad "20" smd rect locked (at -5 5.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp c5a7d9e2-80fa-41c3-ab35-a48b4ee5ecd5))
  (pad "21" smd rect locked (at -5 6.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 2991bfbd-7670-44d7-9c1d-b348247a83da))
  (pad "22" smd rect locked (at -5 8.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 7e73f207-6828-483e-8fa4-ad9e5ce76966))
  (pad "23" smd rect locked (at -5 9.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp addcc87b-7d53-412d-89e9-05e58f04403c))
  (pad "24" smd rect locked (at -5 11.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp a1cf9a61-c853-4b54-9089-09948251fa23))
  (pad "25" smd rect locked (at -5 12.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp e2dfb562-ffb1-48fb-ab2f-4bf3c49b992e))
  (pad "26" smd rect locked (at -5 14.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 99dc36dc-1039-487d-a6cc-9cbb88c54061))
  (pad "27" smd rect locked (at -5 15.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 74d89dfc-aae1-440b-a460-3aad290374a6))
  (pad "28" smd rect locked (at -5 17.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 3c17a4fc-fd4f-4a64-960d-830a02e055ff))
  (pad "29" smd rect locked (at -5 18.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp f11335c1-9df2-43e9-b138-22b44b394b45))
  (pad "30" smd rect locked (at -5 20.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp b4509b43-07b1-44f3-b4ee-1a34f589cd59))
  (pad "31" smd rect locked (at -5 21.75 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 86b0d30b-c7d9-4b59-b406-c903fddd7a14))
  (pad "32" smd rect locked (at -5 23.25 180) (size 5 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 345e3e10-19b2-4c1c-975f-d8e3cea52c36))
  (pad "SHIELD_3" smd rect locked (at 16.25 -13 270) (size 5.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp 631a9b82-02ee-46d5-a462-31839344a01f))
  (pad "SHIELD_4" smd rect locked (at 16.25 13 270) (size 5.5 3.5) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_mask_margin 0.0508) (tstamp affb386f-e6ae-4f99-afcb-5f6b02b3d642))
)
