(footprint "Clock_Generator_Header" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 59FED5CC)
  (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x07 2.54mm single row")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -2.33) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 8e76cb48-5cc8-4230-8363-3ba490a13d0a)
  )
  (fp_text value "Clock_Generator_Header" (at 0 17.57) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 803619fa-8158-4f02-b848-96250671bc9d)
  )
  (fp_text user "CLK0" (at -2.53 15.24 90) (layer "B.SilkS")
    (effects (font (size 0.6 0.6) (thickness 0.15)) (justify mirror))
    (tstamp 0c5de28d-8c4b-4c93-81af-a3e35160e003)
  )
  (fp_text user "SDA" (at -2.53 5.08 90) (layer "B.SilkS")
    (effects (font (size 0.6 0.6) (thickness 0.15)) (justify mirror))
    (tstamp 15dd355e-762a-4fa6-bdf9-5722febb2c23)
  )
  (fp_text user "CLK2" (at -2.53 10.16 90) (layer "B.SilkS")
    (effects (font (size 0.6 0.6) (thickness 0.15)) (justify mirror))
    (tstamp 3e1978c5-d25f-4008-8aec-78b9577a0328)
  )
  (fp_text user "VCC" (at -2.53 0 90) (layer "B.SilkS")
    (effects (font (size 0.6 0.6) (thickness 0.15)) (justify mirror))
    (tstamp 6db27cec-3701-4cc9-8c30-0f31360c182c)
  )
  (fp_text user "GND" (at -2.53 2.54 90) (layer "B.SilkS")
    (effects (font (size 0.6 0.6) (thickness 0.15)) (justify mirror))
    (tstamp 8c5c94d5-17ec-42fd-9ceb-cb847ce8f9fe)
  )
  (fp_text user "CLK1" (at -2.53 12.7 90) (layer "B.SilkS")
    (effects (font (size 0.6 0.6) (thickness 0.15)) (justify mirror))
    (tstamp c210e7ec-fbf5-4e4f-bb29-dc08795b0660)
  )
  (fp_text user "SCL" (at -2.53 7.62 90) (layer "B.SilkS")
    (effects (font (size 0.6 0.6) (thickness 0.15)) (justify mirror))
    (tstamp d7e4a4b1-f400-4c89-9aff-be886186fd6a)
  )
  (fp_text user "1" (at -2.53 12.7 270) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 0674e46d-f95d-49bc-85cf-12421231fe2a)
  )
  (fp_text user "0" (at -2.53 15.24 270) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 4b5a3045-4724-4527-b8e7-66ae8252b1e6)
  )
  (fp_text user "SDA" (at -2.53 5.08 270) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 5696a751-e60a-4a90-ac8f-346df3f96847)
  )
  (fp_text user "GND" (at -2.53 2.54 270) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp 6b933d8f-e806-4905-8bff-1bbe3bd30e3a)
  )
  (fp_text user "CLOCK GENERATOR" (at -5.315 7.62 270) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c2f87a14-3824-417c-ba95-b1fac26a4848)
  )
  (fp_text user "2" (at -2.53 10.16 270) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp c3101509-7514-45a5-97e2-aae0db3cfd7d)
  )
  (fp_text user "VCC" (at -2.53 0 270) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp c4037555-d875-418d-939e-8f3f2831235a)
  )
  (fp_text user "SCL" (at -2.53 7.62 270) (layer "F.SilkS")
    (effects (font (size 0.8 0.8) (thickness 0.15)))
    (tstamp ee90af57-3424-478b-9817-5e74cfe8144b)
  )
  (fp_text user "${REFERENCE}" (at 0 7.62 90) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2a60423e-2737-4a79-aacb-48e99c2086e6)
  )
  (fp_line (start -4.315 0) (end -4.315 15.24) (layer "F.SilkS") (width 0.15) (tstamp 35615647-be58-497b-83c2-34825d999397))
  (fp_line (start -3.8 0) (end -4.315 0) (layer "F.SilkS") (width 0.15) (tstamp b71204e3-514c-458f-ae76-34eacf276202))
  (fp_line (start -4.315 15.24) (end -3.8 15.24) (layer "F.SilkS") (width 0.15) (tstamp ee8f55df-7cee-432a-835f-6ae3fab2fbab))
  (fp_line (start -1.18 16.51) (end 1.18 16.51) (layer "F.CrtYd") (width 0.05) (tstamp 26f116e1-3769-48f2-8d32-68cce2dc8c2d))
  (fp_line (start -1.18 -1.27) (end -1.18 16.51) (layer "F.CrtYd") (width 0.05) (tstamp 3e4bdc11-4439-44e1-8645-dffdeee3095d))
  (fp_line (start -1.18 -1.27) (end 1.18 -1.27) (layer "F.CrtYd") (width 0.05) (tstamp 6a0d93a0-b598-4f06-9377-25160e8373b4))
  (fp_line (start 1.18 16.51) (end 1.18 -1.27) (layer "F.CrtYd") (width 0.05) (tstamp 95d19fc7-a1c1-4dcb-9c2c-9ad3883dff59))
  (fp_line (start -1.18 -0.73) (end -0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp aaf13066-b90c-4e7b-a378-9ce47f78d930))
  (fp_line (start -0.635 -1.27) (end 1.18 -1.27) (layer "F.Fab") (width 0.1) (tstamp af56e90b-a710-470f-8c5f-51e5612b784b))
  (fp_line (start 1.18 16.51) (end -1.18 16.51) (layer "F.Fab") (width 0.1) (tstamp bec6a7df-5703-4394-a2d9-934f3325a8dc))
  (fp_line (start -1.18 16.51) (end -1.18 -0.73) (layer "F.Fab") (width 0.1) (tstamp c8ea947d-50f9-4f5c-92f4-623167229535))
  (fp_line (start 1.18 -1.27) (end 1.18 16.51) (layer "F.Fab") (width 0.1) (tstamp d35746b7-dcde-4cf3-8892-35673c90fa4a))
  (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp c92221b7-e80e-4bcd-b8eb-7b86b4ce2e22))
  (pad "2" thru_hole rect (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp b5ca0c85-3307-4520-8c33-316547d43f87))
  (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 3a83ddcd-c68d-461c-a70c-e73ce6b4cbc2))
  (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp fb5c51a9-e65d-4a12-8682-3466c28aa8e9))
  (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 65681c7e-de16-431d-ba61-aee7cadd5f28))
  (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 34044b43-d5fc-4a88-ac0e-1b4f2c624e08))
  (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp ae856802-b50a-49c8-8fb4-184cc797903e))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
