(footprint "Power_Switch" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "CuK miniature slide switch, OS series, SPDT, right angle, http://www.ckswitches.com/media/1428/os.pdf")
  (tags "switch SPDT")
  (attr through_hole)
  (fp_text reference "REF**" (at 1.4 -3.6) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2845ed75-478f-4a9d-b489-2963e6777b17)
  )
  (fp_text value "Power_Switch" (at 1.7 7.7) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b34f2d11-81ce-4504-8ec0-0c909693ba16)
  )
  (fp_text user "${REFERENCE}" (at 2.3 1.7) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.1)))
    (tstamp 8839c18f-fc8f-4ee3-b424-60948e139511)
  )
  (fp_line (start -2.3 -2.3) (end 6.3 -2.3)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 41f791f7-d18e-4725-b088-1fbb6cb935e3))
  (fp_line (start -2.3 2.3) (end -0.1 2.3)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp ec391758-5041-43bc-b799-821483c3d380))
  (fp_line (start 4 2.3) (end 6.3 2.3)
    (stroke (width 0.15) (type solid)) (layer "F.SilkS") (tstamp 85c89657-f5cd-49c2-9144-3af8c7425087))
  (fp_line (start -3.7 -2.7) (end 7.7 -2.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a51b351e-3aa1-4b46-b922-8337a3681eaf))
  (fp_line (start -3.7 6.7) (end -3.7 -2.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cfd37392-ce49-4e95-927d-7c13c0c57e33))
  (fp_line (start 7.7 -2.7) (end 7.7 6.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b772d040-0423-4b99-aa3e-c037c50daa6c))
  (fp_line (start 7.7 6.7) (end -3.7 6.7)
    (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a08d5f06-7357-42c8-b6dd-cf29b325757d))
  (fp_line (start -2.3 -2.2) (end -2.3 2.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a6861381-8ba4-46b6-9548-279096f31710))
  (fp_line (start -2.3 -2.2) (end 6.3 -2.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d84b622a-a138-487f-b16a-5a53f4d3b5e3))
  (fp_line (start -2.3 2.2) (end 6.3 2.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8fbdb685-a129-4a20-b60a-8c6d45c1eef2))
  (fp_line (start 0 6.2) (end 0 2.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 091056a8-5eaf-4c3b-b6b4-3cf0db59291b))
  (fp_line (start 2 2.2) (end 2 6.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d43810b1-10f6-4e27-a1ce-fb69491b7820))
  (fp_line (start 2 6.2) (end 0 6.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 595c7f70-824b-4d9b-b3e4-b3b92f69c68f))
  (fp_line (start 6.3 2.2) (end 6.3 -2.2)
    (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9ff1a001-e407-4b85-af1f-5e98b37f22ce))
  (pad "" thru_hole circle (at -2.1 0) (size 2.2 2.2) (drill 1.5) (layers "*.Cu" "*.Mask") (tstamp 94c93cb7-7636-48dc-b88d-232c19f163b1))
  (pad "" thru_hole circle (at 6.1 0) (size 2.2 2.2) (drill 1.5) (layers "*.Cu" "*.Mask") (tstamp d7f9772a-23f0-4230-9cad-a1d5908419aa))
  (pad "1" thru_hole oval (at 0 0) (size 1.5 2.5) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp 41b172bb-0908-46ea-909f-e4047e486e2b))
  (pad "2" thru_hole oval (at 2 0) (size 1.5 2.5) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp fedc6201-a345-4643-bc9a-ce8306356cce))
  (pad "3" thru_hole oval (at 4 0) (size 1.5 2.5) (drill 0.9) (layers "*.Cu" "*.Mask") (tstamp 33942096-e624-430f-8e9c-7b0723c2c82e))
  (model "${KIPRJMOD}/../footprints/!OSCR.3dshapes/OS102011MS2Q.wrl"
    (offset (xyz 2 0 0))
    (scale (xyz 0.4 0.4 0.4))
    (rotate (xyz 0 0 0))
  )
)
