(footprint "Cartridge_Port_Adapter-Front" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5A19A42C)
  (descr "Through hole straight socket strip, 1x36, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
  (tags "Through hole socket strip THT 1x36 2.54mm single row")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 -2.77) (layer "F.SilkS") hide
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2f7ef39e-c390-41f0-b1b9-093df297c2b6)
  )
  (fp_text value "Cartridge_Port_Adapter-Front" (at 0 91.67) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7eb873c9-78a3-41a1-8e97-8969f0d4ea82)
  )
  (fp_text user "${REFERENCE}" (at 0 44.45 90) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 258c1ac8-9f95-462b-9b2b-3403b1f9dcf0)
  )
  (fp_line (start -1.18 90.17) (end -1.18 -1.27) (layer "F.CrtYd") (width 0.05) (tstamp 093e9911-2ec4-4bcc-9fa5-0a94b6d57a05))
  (fp_line (start 1.18 -1.27) (end 1.18 90.17) (layer "F.CrtYd") (width 0.05) (tstamp 1c2ef852-ee0c-4815-9a43-ac511d5e45be))
  (fp_line (start -1.18 -1.27) (end 1.18 -1.27) (layer "F.CrtYd") (width 0.05) (tstamp 4542f0ad-4d24-40ab-bdf6-d93f3c584b86))
  (fp_line (start 1.18 90.17) (end -1.18 90.17) (layer "F.CrtYd") (width 0.05) (tstamp b23b809e-8537-4a2e-a7be-b51e703bbacd))
  (fp_line (start 0.635 -1.27) (end 1.18 -0.635) (layer "F.Fab") (width 0.1) (tstamp 034c6d3e-ea54-42ad-a67e-bece56531310))
  (fp_line (start 1.18 90.17) (end -1.18 90.17) (layer "F.Fab") (width 0.1) (tstamp 31047fa0-50e6-4d05-8564-615f8a4e48e8))
  (fp_line (start -1.18 -1.27) (end 0.635 -1.27) (layer "F.Fab") (width 0.1) (tstamp 8cf52205-e314-4cfd-8e04-93bf60a09215))
  (fp_line (start 1.18 -0.635) (end 1.18 90.17) (layer "F.Fab") (width 0.1) (tstamp 91357a75-6821-43cf-ba35-9d9f097d5a2f))
  (fp_line (start -1.18 90.17) (end -1.18 -1.27) (layer "F.Fab") (width 0.1) (tstamp be28449b-415b-40e4-8281-eb8ae0a149df))
  (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 7984faf1-a909-4246-8e9e-886956895dac))
  (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 52c920f6-f414-476e-b963-6daff8106cb8))
  (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 10195b23-a42e-4a01-bbd1-23e0fb0c57bc))
  (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp f7fa5e0e-55ec-4d93-b5bf-23314c8ae041))
  (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp a31cca09-7bdc-421a-a129-cefe11e2d3f2))
  (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 1b67c30e-3549-4b48-b518-19f87bceaf1e))
  (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 71f6cd55-d79f-4512-a876-96d854635f01))
  (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 4c19b955-0023-4a38-ba4f-a03463433a66))
  (pad "9" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 780bf544-3951-4037-b68b-58413b02c76f))
  (pad "10" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 0f036bdf-9e75-4f21-94ea-4be7f2177182))
  (pad "11" thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 53f01676-0595-4479-96ba-ca3a08e9c20d))
  (pad "12" thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 50f7f9b8-3a6b-4ebb-8acd-bebb5e2a5acf))
  (pad "13" thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 80500cf7-8e47-4e41-ab39-19df0d5c1949))
  (pad "14" thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp a4072aee-7ec9-499a-b6a1-650468a67e15))
  (pad "15" thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp a5b18d49-3c43-4cb1-9036-b0bee1fe89c2))
  (pad "16" thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp c95dedd0-f253-4a5c-9623-02b2364801c9))
  (pad "17" thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp ad8b89c7-4c16-4b37-85b5-0557840195a2))
  (pad "18" thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 8ab3f422-3c2f-4512-9584-1d7cde2d6608))
  (pad "19" thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 0bdad5cd-7f14-49b0-b17d-e2eb769d339a))
  (pad "20" thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp edaa03cd-0eba-4c3a-9568-5d26c0f35d5b))
  (pad "21" thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 3577b527-db14-468b-8b89-0f20bf0d5bf2))
  (pad "22" thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 50002eb1-f573-49d5-98aa-2ce5e45778c1))
  (pad "23" thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 4739e6f6-c6f4-442c-bf9d-92a35588cf82))
  (pad "24" thru_hole oval (at 0 58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 2271fbae-a9ec-48e6-aa1d-224eec850074))
  (pad "25" thru_hole oval (at 0 60.96) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp b8ace5c6-fb18-4c43-9afd-5f2f617ffe27))
  (pad "26" thru_hole oval (at 0 63.5) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 082cc178-d179-40db-b653-ba3f64dca5ee))
  (pad "27" thru_hole oval (at 0 66.04) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp c378545b-55d1-4723-aaa6-565cfb2a766d))
  (pad "28" thru_hole oval (at 0 68.58) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 88aac5ab-944f-430d-beb3-6f010425ef18))
  (pad "29" thru_hole oval (at 0 71.12) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp dc95a953-18cf-4452-bc58-3e06a0377574))
  (pad "30" thru_hole oval (at 0 73.66) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 11a6f75c-7604-4ee1-a538-288e39242b82))
  (pad "31" thru_hole oval (at 0 76.2) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp a865631a-661e-4652-8892-5484b516b7c1))
  (pad "32" thru_hole oval (at 0 78.74) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 477f1159-f49b-49bc-a622-1cbfd54a51fa))
  (pad "33" thru_hole oval (at 0 81.28) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp b8f6f4fd-e95e-4aaa-a0e0-b2fe60625ae5))
  (pad "34" thru_hole oval (at 0 83.82) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp 57cf0342-188d-4d15-b9c1-e5043c1c54f7))
  (pad "35" thru_hole oval (at 0 86.36) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp f8539e25-50da-488a-9138-12906897c504))
  (pad "36" thru_hole oval (at 0 88.9) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (tstamp b5beecc4-be93-48d7-bf71-2ffb4e56c826))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x36_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
