# Combined STL file with all parts      

![image](https://dl.dropboxusercontent.com/s/4remnau0kni660i/combined_no_tabs.png?dl=1)   

# Separate STL files for each part    

#### snes_spacer.stl is a small 3d printed spacer to relieve pressure from the pins of SNES clone console slot   

![image](https://dl.dropboxusercontent.com/s/07slhy8pi9ujiri/snes_spacer.png?dl=1)   

#### n64sleeve.stl helps with aligning N64 cartridges if the clone slot is not long/wide enough   
![image](https://dl.dropboxusercontent.com/s/s6jxobazww3sm81/n64sleeve.png?dl=1)   

#### backplate_tabs.stl is the backplate that holds the Arduino    

![image](https://dl.dropboxusercontent.com/s/01v4d28lzbp1ue4/backplate16.png?dl=1)    

#### sd_spacer.stl holds the RGB led and fits between the SD card and the Cart Reader pcb (print with clear PLA/ABS)    

![image](https://dl.dropboxusercontent.com/s/2nujdtcrzvrh7hg/sd_spacer.png?dl=1)  

#### sidewall_tabs.stl secures the Arduino Mega to the backplate with five M2x8 screws    

![image](https://dl.dropboxusercontent.com/s/p7v2l37f1c130b4/sidewall.png?dl=1)  

#### The rest of the STL files are alternative designs in case you use the battery add-on.    

#### Print settings for Slic3r Prusa Edition     
Select the "0.20mm NORMAL" setting that comes with Slic3r and change the following parameters:    
ensure_vertical_shell_thickness = 0     
fill_density = 5%    
first_layer_height = 0.3    
perimeters = 1    
thin_walls = 1    
