<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>FRONT</text>
<wire x1="-45" y1="0.75" x2="-44.2" y2="0" width="0.254" layer="20" curve="90"/>
<wire x1="-44.2" y1="0" x2="-33.2" y2="0" width="0.254" layer="20"/>
<wire x1="-33.2" y1="0" x2="-32.5" y2="0.8" width="0.254" layer="20" curve="90"/>
<wire x1="-32.5" y1="0.8" x2="-32.5" y2="10.5" width="0.254" layer="20"/>
<wire x1="-32.5" y1="10.5" x2="-29.7" y2="10.5" width="0.254" layer="20"/>
<wire x1="-29.7" y1="10.5" x2="-29.7" y2="0.8" width="0.254" layer="20"/>
<wire x1="-29.7" y1="0.8" x2="-29" y2="0" width="0.254" layer="20" curve="90"/>
<wire x1="-29" y1="0" x2="29" y2="0" width="0.254" layer="20"/>
<wire x1="29" y1="0" x2="29.8" y2="0.8" width="0.254" layer="20" curve="90"/>
<wire x1="29.8" y1="0.8" x2="29.8" y2="10.5" width="0.254" layer="20"/>
<wire x1="29.8" y1="10.5" x2="32.5" y2="10.5" width="0.254" layer="20"/>
<wire x1="32.5" y1="10.5" x2="32.5" y2="0.8" width="0.254" layer="20"/>
<wire x1="33.3" y1="0" x2="44.2" y2="0" width="0.254" layer="20"/>
<wire x1="44.2" y1="0" x2="45" y2="0.75" width="0.254" layer="20" curve="90"/>
<wire x1="32.5" y1="0.8" x2="33.3" y2="0" width="0.254" layer="20" curve="90"/>
<wire x1="-50" y1="37.5" x2="-50" y2="36" width="0.254" layer="20"/>
<wire x1="-50" y1="36" x2="-46.85" y2="36.05" width="0.254" layer="20"/>
<wire x1="-46.85" y1="36.05" x2="-46.85" y2="34.05" width="0.254" layer="20"/>
<wire x1="-46.85" y1="34.05" x2="-49.35" y2="34.05" width="0.254" layer="20"/>
<wire x1="-49.35" y1="34.05" x2="-49.35" y2="27.55" width="0.254" layer="20"/>
<wire x1="-49.35" y1="27.55" x2="-49.95" y2="27.55" width="0.254" layer="20"/>
<wire x1="-49.95" y1="27.55" x2="-49.95" y2="17.15" width="0.254" layer="20"/>
<wire x1="-49.95" y1="17.15" x2="-46.85" y2="17.15" width="0.254" layer="20"/>
<wire x1="-46.85" y1="17.15" x2="-46.85" y2="15.15" width="0.254" layer="20"/>
<wire x1="-46.85" y1="15.15" x2="-49.35" y2="15.15" width="0.254" layer="20"/>
<wire x1="-49.35" y1="15.15" x2="-49.35" y2="10.5" width="0.254" layer="20"/>
<wire x1="50.05" y1="10.5" x2="50.05" y2="15.35" width="0.254" layer="20"/>
<wire x1="50.05" y1="15.35" x2="49.05" y2="15.35" width="0.254" layer="20"/>
<wire x1="49.05" y1="15.35" x2="49.05" y2="20.45" width="0.254" layer="20"/>
<wire x1="49.05" y1="20.45" x2="46.55" y2="20.45" width="0.254" layer="20"/>
<wire x1="46.55" y1="20.45" x2="46.55" y2="22.45" width="0.254" layer="20"/>
<wire x1="46.55" y1="22.45" x2="49.05" y2="22.45" width="0.254" layer="20"/>
<wire x1="49.05" y1="22.45" x2="49.05" y2="25.75" width="0.254" layer="20"/>
<wire x1="49.05" y1="25.75" x2="46.85" y2="25.75" width="0.254" layer="20"/>
<wire x1="46.85" y1="25.75" x2="46.85" y2="27.75" width="0.254" layer="20"/>
<wire x1="46.85" y1="27.75" x2="50" y2="27.75" width="0.254" layer="20"/>
<wire x1="50" y1="27.75" x2="50" y2="37.5" width="0.254" layer="20"/>
<wire x1="45" y1="0.75" x2="45" y2="10.5" width="0.254" layer="20"/>
<wire x1="45" y1="10.5" x2="50.05" y2="10.5" width="0.254" layer="20"/>
<wire x1="-45" y1="0.75" x2="-45" y2="10.5" width="0.254" layer="20"/>
<wire x1="-45" y1="10.5" x2="-49.35" y2="10.5" width="0.254" layer="20"/>
<text>FAMICOM TO SNES
     ADAPTER</text>
<text>30</text>
<text>1</text>
<text>60</text>
<text>31</text>
<wire x1="50" y1="37.5" x2="-50" y2="37.5" width="0.254" layer="20"/>
</plain>
<libraries>
<library name="snes_cart_mod4">
<description>&lt;b&gt;SNES Cartridge Part Library&lt;/b&gt;&lt;p&gt;

Contains board outlines and common chips used in Super Nintendo game cartridges.
&lt;ul&gt;
&lt;li&gt;MaskROM
&lt;li&gt;SRAM
&lt;li&gt;Address Decoder
&lt;li&gt;Lockout chip
&lt;/ul&gt;
Also contains many chips used in reproduction cartridges.
&lt;ul&gt;
&lt;li&gt;Flash ROM
&lt;li&gt;SuperCIC lockout chip clone
&lt;/ul&gt;
&lt;author&gt;Created by qwertymodo&lt;/author&gt;&lt;p&gt;

Additional parts added by magno:
&lt;ul&gt;
&lt;li&gt;32Mbit UV EPROM
&lt;li&gt;Various 74XXX decoders
&lt;/ul&gt;

&lt;p&gt;
Email: qwertymodo@gmail.com</description>
<packages>
<package name="CART-EXP-PINS-LONG">
</package>
</packages>
</library>
<library name="!sanni_mod3">
<packages>
<package name="FAMICOM_PINS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="snes_cart_mod4" package="CART-EXP-PINS-LONG" value="CART-EXP-EDGE"/>
<element name="U$2" library="!sanni_mod3" package="FAMICOM_PINS" value="FAMICOM-CART_PINS"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="36"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$2" pad="16"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="27"/>
<contactref element="U$1" pad="58"/>
<contactref element="U$2" pad="31"/>
<contactref element="U$2" pad="30"/>
</signal>
<signal name="PPU_RD">
<contactref element="U$1" pad="12"/>
<contactref element="U$2" pad="17"/>
</signal>
<signal name="A6">
<contactref element="U$1" pad="47"/>
<contactref element="U$2" pad="7"/>
<contactref element="U$2" pad="19"/>
</signal>
<signal name="A5">
<contactref element="U$1" pad="46"/>
<contactref element="U$2" pad="8"/>
<contactref element="U$2" pad="20"/>
</signal>
<signal name="A3">
<contactref element="U$1" pad="44"/>
<contactref element="U$2" pad="10"/>
<contactref element="U$2" pad="22"/>
</signal>
<signal name="A2">
<contactref element="U$1" pad="43"/>
<contactref element="U$2" pad="11"/>
<contactref element="U$2" pad="23"/>
</signal>
<signal name="A0">
<contactref element="U$1" pad="41"/>
<contactref element="U$2" pad="13"/>
<contactref element="U$2" pad="25"/>
</signal>
<signal name="D7">
<contactref element="U$1" pad="40"/>
<contactref element="U$2" pad="36"/>
<contactref element="U$2" pad="57"/>
</signal>
<signal name="D5">
<contactref element="U$1" pad="38"/>
<contactref element="U$2" pad="38"/>
<contactref element="U$2" pad="59"/>
</signal>
<signal name="A13">
<contactref element="U$1" pad="61"/>
<contactref element="U$2" pad="34"/>
<contactref element="U$2" pad="56"/>
</signal>
<signal name="A11">
<contactref element="U$1" pad="60"/>
<contactref element="U$2" pad="54"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="M2">
<contactref element="U$1" pad="17"/>
<contactref element="U$2" pad="32"/>
</signal>
<signal name="CIRAM_CE">
<contactref element="U$1" pad="14"/>
<contactref element="U$2" pad="48"/>
</signal>
<signal name="IRQ">
<contactref element="U$1" pad="11"/>
<contactref element="U$2" pad="15"/>
</signal>
<signal name="CPU_RW">
<contactref element="U$1" pad="10"/>
<contactref element="U$2" pad="14"/>
</signal>
<signal name="D1">
<contactref element="U$1" pad="8"/>
<contactref element="U$2" pad="42"/>
<contactref element="U$2" pad="27"/>
</signal>
<signal name="D3">
<contactref element="U$1" pad="6"/>
<contactref element="U$2" pad="40"/>
<contactref element="U$2" pad="29"/>
</signal>
<signal name="A14">
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="35"/>
</signal>
<signal name="A12">
<contactref element="U$1" pad="30"/>
<contactref element="U$2" pad="33"/>
<contactref element="U$2" pad="55"/>
</signal>
<signal name="A8">
<contactref element="U$1" pad="28"/>
<contactref element="U$2" pad="51"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="D0">
<contactref element="U$1" pad="9"/>
<contactref element="U$2" pad="43"/>
<contactref element="U$2" pad="26"/>
</signal>
<signal name="D2">
<contactref element="U$1" pad="7"/>
<contactref element="U$2" pad="41"/>
<contactref element="U$2" pad="28"/>
</signal>
<signal name="D4">
<contactref element="U$1" pad="37"/>
<contactref element="U$2" pad="39"/>
<contactref element="U$2" pad="60"/>
</signal>
<signal name="D6">
<contactref element="U$1" pad="39"/>
<contactref element="U$2" pad="37"/>
<contactref element="U$2" pad="58"/>
</signal>
<signal name="A1">
<contactref element="U$1" pad="42"/>
<contactref element="U$2" pad="12"/>
<contactref element="U$2" pad="24"/>
</signal>
<signal name="A4">
<contactref element="U$1" pad="45"/>
<contactref element="U$2" pad="9"/>
<contactref element="U$2" pad="21"/>
</signal>
<signal name="A7">
<contactref element="U$1" pad="48"/>
<contactref element="U$2" pad="50"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="A9">
<contactref element="U$1" pad="59"/>
<contactref element="U$2" pad="52"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="A10">
<contactref element="U$1" pad="29"/>
<contactref element="U$2" pad="53"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="CIRAM_A10">
<contactref element="U$1" pad="21"/>
<contactref element="U$2" pad="18"/>
</signal>
<signal name="ROMSEL">
<contactref element="U$1" pad="16"/>
<contactref element="U$2" pad="44"/>
</signal>
<signal name="PPU_WR">
<contactref element="U$1" pad="15"/>
<contactref element="U$2" pad="47"/>
</signal>
<signal name="!PPU_A13">
<contactref element="U$1" pad="13"/>
<contactref element="U$2" pad="49"/>
</signal>
<signal name="N$28">
</signal>
</signals>
</board>
</drawing>
</eagle>
