{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["NDS_TV_OUT_V1I2"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"NDS_TV_OUT_V1I2","index":0,"n_rows":18,"n_cols":8,"rows_kept":18}
["Comment","Description","Designator","Footprint","LibRef","Quantity","Manufacturer Part Number"]
["MAX5184BEEG+","DAC 1-CH Current Steering 10-bit 24-Pin QSOP","U1","SOP63P602X175-24N","MAX5184BEEG+",1,"MAX5184BEEG+"]
["MAX4414ESA+","IC OPAMP VFB 400MHZ RRO 8SOIC","U2","SOIC127P600X175-8N","MAX4414ESA+",1,"MAX4414ESA+"]
["KLPX-0848A-2-Y","Conn RCA F 2 POS 4.5mm Solder RA Thru-Hole 2 Terminal 1 Port","J4","KLPX0848A2Y","KLPX-0848A-2-Y",1,"KLPX-0848A-2-Y"]
["KLPX-0848A-2-W","Conn RCA F 2 POS 4.5mm Solder RA Thru-Hole 2 Terminal 1 Port","J2","KLPX0848A2W","KLPX-0848A-2-W",1,"KLPX-0848A-2-W"]
["KLPX-0848A-2-R","Conn RCA F 2 POS 4.5mm Solder RA Thru-Hole 2 Terminal 1 Port","J3","KLPX0848A2R","KLPX-0848A-2-R",1,"KLPX-0848A-2-R"]
["JS102011SAQN","Slide Switch, JS Series, SPDT, Right Angle, SMD, 100 mA ;RoHS Compliant: Yes","S4","SW_JS102011SAQN","JS102011SAQN",1,"JS102011SAQN"]
["DNP","","R2, R4","R0603","R0603",2]
["B3U-1000P","SWITCH TACTILE SPST-NO 0.05A 12V","S1, S2, S3","SW_B3U-1000P","B3U-1000P",3,"B3U-1000P"]
["APTD1608LZGCK","LED GREEN CLEAR 0603 SMD","LED1","RESC0603X55N","APTD1608LZGCK",1,"APTD1608LZGCK"]
["430R","Res, 430R, 0.1%, 0.1W, 0603, Thin Film","R3","R0603","MCWF06R4300BTL",1,"MCWF06R4300BTL"]
["320R","High Precision-High Stability Chip Resistor Thin Film 0603 320Ohm 0.5% Paper T/R","R6","R0603","RT0603DRE07320RL",1,"RT0603DRE07320RL"]
["75R","VISHAY - CRCW060375R0FKEA - RES, 75R, 1%, 0.1W, 0603, THICK FILM","R1","R0603","RC0603FR-0775RL",1,"RC0603FR-0775RL"]
["10uF","CAPACITOR, CASE A, 10UF, 10V; Product Range:KEMET - T491 Series; Capacitance:10µF; Capacitance Tolerance:± 10%; Voltage Rating:10V; Capacitor Case Style:1206 [3216 Metric]; Manufacturer Size Code:A; Operating Temperature Max:125°C; ;RoHS Compliant: Yes","C1, C2","C1206T","T491A106K010AT",2,"T491A106K010AT"]
["4-2328724-5","FPC Connector; 0.3mm pitch front flip FPC; 45pos","J1","423287245","4-2328724-5",1,"4-2328724-5"]
["1K","ROHM - ESR03EZPF1001 - SMD Chip Resistor, Anti-Surge, 0603 [1608 Metric], 1 kohm, ESR Series, 150 V, Thick Film, 250 mW","R5, R7","R0603","ESR03EZPF1001",2,"ESR03EZPF1001"]
["0.1uF","MURATA - GRM319R71H104KA01D - COND, CERÁ MULT, X7R, 100NF, 50V, 1206","C3, C4, C5, C6, C7","C1206","C1206C104K5RAC7210",5,"C1206C104K5RAC7210"]
["Ribbon Cable FPC 0,3mm pitch 45 pin",{"$nulls":4},1,"https://es.aliexpress.com/item/4000499971802.html?spm=a2g0s.9042311.0.0.415d63c0FOSqsK","https://www.mouser.es/Wire-Cable/FFC-FPC-Jumper-Cables/_/N-ad930?P=1y9j0ziZ1z0wxp5"]