<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>Collection of parts used in SummerCart64 design</description>
<packages>
<package name="EQFP144">
</package>
<package name="N64_EDGE">
<description>Footprint for Nintendo 64 cartridge edge connector.</description>
</package>
<package name="MICRO_USB">
</package>
<package name="MICRO_SD">
</package>
<package name="TSSOP8">
</package>
<package name="SO8_150MIL">
</package>
<package name="SO8_208MIL">
</package>
<package name="3.2X2.5_OSCILLATOR">
</package>
<package name="LQFP64">
</package>
<package name="218-2">
</package>
</packages>
<symbols>
<symbol name="MAX10EQFP144_BANK_1A">
<pin name="1A_6"/>
<pin name="1A_7"/>
<pin name="1A_8"/>
<pin name="1A_10"/>
<pin name="1A_11"/>
<pin name="1A_12"/>
<pin name="1A_13"/>
<pin name="1A_14"/>
<pin name="VCCIO1A" direction="pwr"/>
</symbol>
<symbol name="MAX10EQFP144_BANK_1B">
<pin name="JTAGEN/1B_15"/>
<pin name="TMS/1B_16"/>
<pin name="VREFB1N0/1B_17"/>
<pin name="TCK/1B_18" function="clk"/>
<pin name="TDI/1B_19"/>
<pin name="TDO/1B_20"/>
<pin name="1B_21"/>
<pin name="1B_22"/>
<pin name="1B_24"/>
<pin name="1B_25"/>
<pin name="VCCIO1B" direction="pwr"/>
</symbol>
<symbol name="MAX10EQFP144_BANK_2">
<pin name="CLK0N/2_26" function="dotclk"/>
<pin name="CLK0P/2_27" function="clk"/>
<pin name="CLK1N/2_28" function="dotclk"/>
<pin name="CLK1P/2_29" function="clk"/>
<pin name="VREFB2N0/2_30"/>
<pin name="PLL_L_CLKOUTN/2_32" function="dot"/>
<pin name="PLL_L_CLKOUTP/2_33"/>
<pin name="VCCIO2" direction="pwr"/>
</symbol>
<symbol name="MAX10EQFP144_BANK_3">
<pin name="3_38"/>
<pin name="3_39"/>
<pin name="3_41"/>
<pin name="3_43"/>
<pin name="3_44"/>
<pin name="3_45"/>
<pin name="3_46"/>
<pin name="3_47"/>
<pin name="3_50"/>
<pin name="VREFB3N0/3_48"/>
<pin name="3_52"/>
<pin name="3_54"/>
<pin name="3_55"/>
<pin name="3_56"/>
<pin name="3_57"/>
<pin name="3_58"/>
<pin name="3_59"/>
<pin name="3_60"/>
<pin name="VCCIO3@1" direction="pwr"/>
<pin name="VCCIO3@2" direction="pwr"/>
</symbol>
<symbol name="MAX10EQFP144_BANK_4">
<pin name="VREFB4N0/4_61"/>
<pin name="4_62"/>
<pin name="4_64"/>
<pin name="4_65"/>
<pin name="4_66"/>
<pin name="4_69"/>
<pin name="4_70"/>
<pin name="VCCIO4" direction="pwr"/>
</symbol>
<symbol name="MAX10EQFP144_BANK_5">
<pin name="5_75"/>
<pin name="5_74"/>
<pin name="5_77"/>
<pin name="5_76"/>
<pin name="5_79"/>
<pin name="5_78"/>
<pin name="5_81"/>
<pin name="5_85"/>
<pin name="5_84"/>
<pin name="5_87"/>
<pin name="5_86"/>
<pin name="VREFB5N0/5_80"/>
<pin name="VCCIO5" direction="pwr"/>
</symbol>
<symbol name="MAX10EQFP144_BANK_6">
<pin name="CLK2P/6_88" function="clk"/>
<pin name="CLK2N/6_89" function="dotclk"/>
<pin name="CLK3P/6_90" function="clk"/>
<pin name="CLK3N/6_91" function="dotclk"/>
<pin name="6_92"/>
<pin name="6_93"/>
<pin name="DPCLK3/6_96" function="clk"/>
<pin name="DPCLK2/6_98" function="clk"/>
<pin name="6_99"/>
<pin name="6_100"/>
<pin name="6_101"/>
<pin name="6_102"/>
<pin name="6_105"/>
<pin name="6_106"/>
<pin name="VREFB6N0/6_97"/>
<pin name="VCCIO6@1" direction="pwr"/>
<pin name="VCCIO6@2" direction="pwr"/>
</symbol>
<symbol name="MAX10EQFP144_BANK_7">
<pin name="7_110"/>
<pin name="7_111"/>
<pin name="7_113"/>
<pin name="7_114"/>
<pin name="7_118"/>
<pin name="7_119"/>
<pin name="VREFB7N0/7_112"/>
<pin name="VCCIO7" direction="pwr"/>
</symbol>
<symbol name="MAX10EQFP144_BANK_8">
<pin name="8_120"/>
<pin name="DEV_CLRN/8_121" function="dot"/>
<pin name="DEV_OE/8_122"/>
<pin name="CONFIG_SEL/8_126"/>
<pin name="8_124"/>
<pin name="NCONFIG/8_129" direction="in" function="dot"/>
<pin name="8_127"/>
<pin name="8_130"/>
<pin name="8_131"/>
<pin name="8_132"/>
<pin name="CRC_ERROR/8_134"/>
<pin name="8_135"/>
<pin name="NSTATUS/8_136" function="dot"/>
<pin name="CONF_DONE/8_138"/>
<pin name="8_140"/>
<pin name="8_141"/>
<pin name="VREFB8N0/8_123"/>
<pin name="VCCIO8@1" direction="pwr"/>
<pin name="VCCIO8@2" direction="pwr"/>
</symbol>
<symbol name="MAX10EQFP144_PWR">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="VCCA1" direction="pwr"/>
<pin name="VCCA2" direction="pwr"/>
<pin name="VCCA3@1" direction="pwr"/>
<pin name="VCCA4" direction="pwr"/>
<pin name="VCCA5" direction="pwr"/>
<pin name="VCCA6" direction="pwr"/>
<pin name="VCC_ONE@1" direction="pwr"/>
<pin name="VCC_ONE@2" direction="pwr"/>
<pin name="VCC_ONE@3" direction="pwr"/>
<pin name="VCC_ONE@4" direction="pwr"/>
<pin name="VCC_ONE@5" direction="pwr"/>
<pin name="VCC_ONE@6" direction="pwr"/>
<pin name="VCC_ONE@7" direction="pwr"/>
<pin name="VCC_ONE@8" direction="pwr"/>
<pin name="VCC_ONE@9" direction="pwr"/>
<pin name="VCC_ONE@10" direction="pwr"/>
<pin name="VCCA3@2" direction="pwr"/>
<pin name="GND@CASE_T" direction="pwr"/>
<pin name="GND@CASE_B" direction="pwr"/>
</symbol>
<symbol name="N64_EDGE">
<description>Symbol for Nintendo 64 cartridge edge connector.</description>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="AD15"/>
<pin name="AD14"/>
<pin name="AD13"/>
<pin name="GND@6" direction="pwr"/>
<pin name="AD12"/>
<pin name="/WRITE" direction="out" function="dot"/>
<pin name="3V3@9" direction="pwr"/>
<pin name="/READ" direction="out" function="dot"/>
<pin name="AD11"/>
<pin name="AD10"/>
<pin name="12V@13" direction="pwr"/>
<pin name="KEY@14" direction="nc"/>
<pin name="AD9"/>
<pin name="AD8"/>
<pin name="3V3@17" direction="pwr"/>
<pin name="CIC_DATA_IO"/>
<pin name="SI_CLK" direction="out" function="clk"/>
<pin name="/RESET" direction="out" function="dot"/>
<pin name="SI_DATA"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="LAUDIO" direction="in"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="GND@31" direction="pwr"/>
<pin name="AD3"/>
<pin name="ALEL" direction="out"/>
<pin name="3V3@34" direction="pwr"/>
<pin name="ALEH" direction="out"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="12V@38" direction="pwr"/>
<pin name="KEY@39" direction="nc"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="3V3@42" direction="pwr"/>
<pin name="CIC_DATA_CLK" direction="out"/>
<pin name="JTCK" direction="in"/>
<pin name="/NMI" direction="out" function="dot"/>
<pin name="VIDEO_SYNC" direction="out"/>
<pin name="GND@47" direction="pwr"/>
<pin name="GND@48" direction="pwr"/>
<pin name="RAUDIO" direction="in"/>
<pin name="GND@50" direction="pwr"/>
</symbol>
<symbol name="MICRO_USB">
<pin name="+5V" direction="pwr"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="ID"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
</symbol>
<symbol name="MICRO_SD">
<pin name="GND@6" direction="pwr"/>
<pin name="GND@G1" direction="pwr"/>
<pin name="GND@G2" direction="pwr"/>
<pin name="GND@G3" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND@G4" direction="pwr"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CMD"/>
<pin name="DAT0"/>
<pin name="DAT1"/>
<pin name="DAT2"/>
<pin name="DAT3"/>
<pin name="CD1"/>
<pin name="CD2"/>
</symbol>
<symbol name="93CX6">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="D" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="C" direction="in" function="clk"/>
<pin name="S" direction="in"/>
<pin name="ORG" direction="in"/>
<pin name="DU" direction="nc"/>
</symbol>
<symbol name="ATTINYX5">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="MOSI/PB0"/>
<pin name="MISO/PB1"/>
<pin name="SCK/PB2"/>
<pin name="CLKI/PB3" function="clk"/>
<pin name="CLKO/PB4"/>
<pin name="RESET/PB5" function="dot"/>
</symbol>
<symbol name="SPI_MEMORY">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="/CS" direction="in"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="SIO0"/>
<pin name="SIO1"/>
<pin name="SIO2"/>
<pin name="SIO3"/>
</symbol>
<symbol name="OSC">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="OUT2/NC" direction="out"/>
<pin name="EN/NC" direction="in"/>
</symbol>
<symbol name="MCP7940N">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="X1"/>
<pin name="X2"/>
<pin name="VBAT" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="MFP"/>
</symbol>
<symbol name="FT2232H">
<pin name="VREGIN" direction="pwr"/>
<pin name="VREGOUT" direction="pwr"/>
<pin name="DM"/>
<pin name="DP"/>
<pin name="REF" direction="in"/>
<pin name="RESET#" direction="in"/>
<pin name="EECS"/>
<pin name="EECLK" direction="out"/>
<pin name="EEDATA"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="TEST" direction="in"/>
<pin name="VPHY" direction="pwr"/>
<pin name="VPLL" direction="pwr"/>
<pin name="VCORE@12" direction="pwr"/>
<pin name="VCORE@64" direction="pwr"/>
<pin name="VCORE@37" direction="pwr"/>
<pin name="VCCIO@20" direction="pwr"/>
<pin name="VCCIO@31" direction="pwr"/>
<pin name="VCCIO@42" direction="pwr"/>
<pin name="VCCIO@56" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@35" direction="pwr"/>
<pin name="GND@47" direction="pwr"/>
<pin name="GND@51" direction="pwr"/>
<pin name="SUSPEND#" direction="out"/>
<pin name="PWREN#" direction="out"/>
<pin name="ADBUS0"/>
<pin name="ADBUS1"/>
<pin name="ADBUS2"/>
<pin name="ADBUS3"/>
<pin name="ADBUS4"/>
<pin name="ADBUS5"/>
<pin name="ADBUS6"/>
<pin name="ADBUS7"/>
<pin name="ACBUS0"/>
<pin name="ACBUS1"/>
<pin name="ACBUS2"/>
<pin name="ACBUS3"/>
<pin name="ACBUS4"/>
<pin name="ACBUS5"/>
<pin name="ACBUS6"/>
<pin name="ACBUS7"/>
<pin name="BDBUS0"/>
<pin name="BDBUS1"/>
<pin name="BDBUS2"/>
<pin name="BDBUS3"/>
<pin name="BDBUS4"/>
<pin name="BDBUS5"/>
<pin name="BDBUS6"/>
<pin name="BDBUS7"/>
<pin name="BCBUS0"/>
<pin name="BCBUS1"/>
<pin name="BCBUS2"/>
<pin name="BCBUS3"/>
<pin name="BCBUS4"/>
<pin name="BCBUS5"/>
<pin name="BCBUS6"/>
<pin name="BCBUS7"/>
</symbol>
<symbol name="SWITCH-2">
<pin name="4"/>
<pin name="3"/>
<pin name="2"/>
<pin name="1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="10M08SCE144C8G" prefix="U">
<gates>
<gate name="A" symbol="MAX10EQFP144_BANK_1A"/>
<gate name="B" symbol="MAX10EQFP144_BANK_1B"/>
<gate name="C" symbol="MAX10EQFP144_BANK_2"/>
<gate name="D" symbol="MAX10EQFP144_BANK_3"/>
<gate name="E" symbol="MAX10EQFP144_BANK_4"/>
<gate name="F" symbol="MAX10EQFP144_BANK_5"/>
<gate name="G" symbol="MAX10EQFP144_BANK_6"/>
<gate name="H" symbol="MAX10EQFP144_BANK_7"/>
<gate name="I" symbol="MAX10EQFP144_BANK_8"/>
<gate name="J" symbol="MAX10EQFP144_PWR"/>
</gates>
<devices>
<device name="" package="EQFP144">
<connects>
<connect gate="A" pin="1A_10" pad="10"/>
<connect gate="A" pin="1A_11" pad="11"/>
<connect gate="A" pin="1A_12" pad="12"/>
<connect gate="A" pin="1A_13" pad="13"/>
<connect gate="A" pin="1A_14" pad="14"/>
<connect gate="A" pin="1A_6" pad="6"/>
<connect gate="A" pin="1A_7" pad="7"/>
<connect gate="A" pin="1A_8" pad="8"/>
<connect gate="A" pin="VCCIO1A" pad="9"/>
<connect gate="B" pin="1B_21" pad="21"/>
<connect gate="B" pin="1B_22" pad="22"/>
<connect gate="B" pin="1B_24" pad="24"/>
<connect gate="B" pin="1B_25" pad="25"/>
<connect gate="B" pin="JTAGEN/1B_15" pad="15"/>
<connect gate="B" pin="TCK/1B_18" pad="18"/>
<connect gate="B" pin="TDI/1B_19" pad="19"/>
<connect gate="B" pin="TDO/1B_20" pad="20"/>
<connect gate="B" pin="TMS/1B_16" pad="16"/>
<connect gate="B" pin="VCCIO1B" pad="23"/>
<connect gate="B" pin="VREFB1N0/1B_17" pad="17"/>
<connect gate="C" pin="CLK0N/2_26" pad="26"/>
<connect gate="C" pin="CLK0P/2_27" pad="27"/>
<connect gate="C" pin="CLK1N/2_28" pad="28"/>
<connect gate="C" pin="CLK1P/2_29" pad="29"/>
<connect gate="C" pin="PLL_L_CLKOUTN/2_32" pad="32"/>
<connect gate="C" pin="PLL_L_CLKOUTP/2_33" pad="33"/>
<connect gate="C" pin="VCCIO2" pad="31"/>
<connect gate="C" pin="VREFB2N0/2_30" pad="30"/>
<connect gate="D" pin="3_38" pad="38"/>
<connect gate="D" pin="3_39" pad="39"/>
<connect gate="D" pin="3_41" pad="41"/>
<connect gate="D" pin="3_43" pad="43"/>
<connect gate="D" pin="3_44" pad="44"/>
<connect gate="D" pin="3_45" pad="45"/>
<connect gate="D" pin="3_46" pad="46"/>
<connect gate="D" pin="3_47" pad="47"/>
<connect gate="D" pin="3_50" pad="50"/>
<connect gate="D" pin="3_52" pad="52"/>
<connect gate="D" pin="3_54" pad="54"/>
<connect gate="D" pin="3_55" pad="55"/>
<connect gate="D" pin="3_56" pad="56"/>
<connect gate="D" pin="3_57" pad="57"/>
<connect gate="D" pin="3_58" pad="58"/>
<connect gate="D" pin="3_59" pad="59"/>
<connect gate="D" pin="3_60" pad="60"/>
<connect gate="D" pin="VCCIO3@1" pad="49"/>
<connect gate="D" pin="VCCIO3@2" pad="40"/>
<connect gate="D" pin="VREFB3N0/3_48" pad="48"/>
<connect gate="E" pin="4_62" pad="62"/>
<connect gate="E" pin="4_64" pad="64"/>
<connect gate="E" pin="4_65" pad="65"/>
<connect gate="E" pin="4_66" pad="66"/>
<connect gate="E" pin="4_69" pad="69"/>
<connect gate="E" pin="4_70" pad="70"/>
<connect gate="E" pin="VCCIO4" pad="67"/>
<connect gate="E" pin="VREFB4N0/4_61" pad="61"/>
<connect gate="F" pin="5_74" pad="74"/>
<connect gate="F" pin="5_75" pad="75"/>
<connect gate="F" pin="5_76" pad="76"/>
<connect gate="F" pin="5_77" pad="77"/>
<connect gate="F" pin="5_78" pad="78"/>
<connect gate="F" pin="5_79" pad="79"/>
<connect gate="F" pin="5_81" pad="81"/>
<connect gate="F" pin="5_84" pad="84"/>
<connect gate="F" pin="5_85" pad="85"/>
<connect gate="F" pin="5_86" pad="86"/>
<connect gate="F" pin="5_87" pad="87"/>
<connect gate="F" pin="VCCIO5" pad="82"/>
<connect gate="F" pin="VREFB5N0/5_80" pad="80"/>
<connect gate="G" pin="6_100" pad="100"/>
<connect gate="G" pin="6_101" pad="101"/>
<connect gate="G" pin="6_102" pad="102"/>
<connect gate="G" pin="6_105" pad="105"/>
<connect gate="G" pin="6_106" pad="106"/>
<connect gate="G" pin="6_92" pad="92"/>
<connect gate="G" pin="6_93" pad="93"/>
<connect gate="G" pin="6_99" pad="99"/>
<connect gate="G" pin="CLK2N/6_89" pad="89"/>
<connect gate="G" pin="CLK2P/6_88" pad="88"/>
<connect gate="G" pin="CLK3N/6_91" pad="91"/>
<connect gate="G" pin="CLK3P/6_90" pad="90"/>
<connect gate="G" pin="DPCLK2/6_98" pad="98"/>
<connect gate="G" pin="DPCLK3/6_96" pad="96"/>
<connect gate="G" pin="VCCIO6@1" pad="94"/>
<connect gate="G" pin="VCCIO6@2" pad="103"/>
<connect gate="G" pin="VREFB6N0/6_97" pad="97"/>
<connect gate="H" pin="7_110" pad="110"/>
<connect gate="H" pin="7_111" pad="111"/>
<connect gate="H" pin="7_113" pad="113"/>
<connect gate="H" pin="7_114" pad="114"/>
<connect gate="H" pin="7_118" pad="118"/>
<connect gate="H" pin="7_119" pad="119"/>
<connect gate="H" pin="VCCIO7" pad="117"/>
<connect gate="H" pin="VREFB7N0/7_112" pad="112"/>
<connect gate="I" pin="8_120" pad="120"/>
<connect gate="I" pin="8_124" pad="124"/>
<connect gate="I" pin="8_127" pad="127"/>
<connect gate="I" pin="8_130" pad="130"/>
<connect gate="I" pin="8_131" pad="131"/>
<connect gate="I" pin="8_132" pad="132"/>
<connect gate="I" pin="8_135" pad="135"/>
<connect gate="I" pin="8_140" pad="140"/>
<connect gate="I" pin="8_141" pad="141"/>
<connect gate="I" pin="CONFIG_SEL/8_126" pad="126"/>
<connect gate="I" pin="CONF_DONE/8_138" pad="138"/>
<connect gate="I" pin="CRC_ERROR/8_134" pad="134"/>
<connect gate="I" pin="DEV_CLRN/8_121" pad="121"/>
<connect gate="I" pin="DEV_OE/8_122" pad="122"/>
<connect gate="I" pin="NCONFIG/8_129" pad="129"/>
<connect gate="I" pin="NSTATUS/8_136" pad="136"/>
<connect gate="I" pin="VCCIO8@1" pad="139"/>
<connect gate="I" pin="VCCIO8@2" pad="128"/>
<connect gate="I" pin="VREFB8N0/8_123" pad="123"/>
<connect gate="J" pin="GND@1" pad="3"/>
<connect gate="J" pin="GND@10" pad="137"/>
<connect gate="J" pin="GND@11" pad="133"/>
<connect gate="J" pin="GND@12" pad="125"/>
<connect gate="J" pin="GND@13" pad="116"/>
<connect gate="J" pin="GND@14" pad="104"/>
<connect gate="J" pin="GND@2" pad="4"/>
<connect gate="J" pin="GND@3" pad="95"/>
<connect gate="J" pin="GND@4" pad="83"/>
<connect gate="J" pin="GND@5" pad="68"/>
<connect gate="J" pin="GND@6" pad="63"/>
<connect gate="J" pin="GND@7" pad="53"/>
<connect gate="J" pin="GND@8" pad="42"/>
<connect gate="J" pin="GND@9" pad="142"/>
<connect gate="J" pin="GND@CASE_B" pad="CASE_B"/>
<connect gate="J" pin="GND@CASE_T" pad="CASE_T"/>
<connect gate="J" pin="VCCA1" pad="35"/>
<connect gate="J" pin="VCCA2" pad="34"/>
<connect gate="J" pin="VCCA3@1" pad="5"/>
<connect gate="J" pin="VCCA3@2" pad="107"/>
<connect gate="J" pin="VCCA4" pad="143"/>
<connect gate="J" pin="VCCA5" pad="71"/>
<connect gate="J" pin="VCCA6" pad="2"/>
<connect gate="J" pin="VCC_ONE@1" pad="73"/>
<connect gate="J" pin="VCC_ONE@10" pad="1"/>
<connect gate="J" pin="VCC_ONE@2" pad="72"/>
<connect gate="J" pin="VCC_ONE@3" pad="51"/>
<connect gate="J" pin="VCC_ONE@4" pad="37"/>
<connect gate="J" pin="VCC_ONE@5" pad="36"/>
<connect gate="J" pin="VCC_ONE@6" pad="144"/>
<connect gate="J" pin="VCC_ONE@7" pad="115"/>
<connect gate="J" pin="VCC_ONE@8" pad="109"/>
<connect gate="J" pin="VCC_ONE@9" pad="108"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="N64_EDGE" prefix="J">
<description>Nintendo 64 cartridge edge connector.</description>
<gates>
<gate name="&gt;NAME" symbol="N64_EDGE"/>
</gates>
<devices>
<device name="" package="N64_EDGE">
<connects>
<connect gate="&gt;NAME" pin="/NMI" pad="45"/>
<connect gate="&gt;NAME" pin="/READ" pad="10"/>
<connect gate="&gt;NAME" pin="/RESET" pad="20"/>
<connect gate="&gt;NAME" pin="/WRITE" pad="8"/>
<connect gate="&gt;NAME" pin="12V@13" pad="13"/>
<connect gate="&gt;NAME" pin="12V@38" pad="38"/>
<connect gate="&gt;NAME" pin="3V3@17" pad="17"/>
<connect gate="&gt;NAME" pin="3V3@34" pad="34"/>
<connect gate="&gt;NAME" pin="3V3@42" pad="42"/>
<connect gate="&gt;NAME" pin="3V3@9" pad="9"/>
<connect gate="&gt;NAME" pin="AD0" pad="28"/>
<connect gate="&gt;NAME" pin="AD1" pad="29"/>
<connect gate="&gt;NAME" pin="AD10" pad="12"/>
<connect gate="&gt;NAME" pin="AD11" pad="11"/>
<connect gate="&gt;NAME" pin="AD12" pad="7"/>
<connect gate="&gt;NAME" pin="AD13" pad="5"/>
<connect gate="&gt;NAME" pin="AD14" pad="4"/>
<connect gate="&gt;NAME" pin="AD15" pad="3"/>
<connect gate="&gt;NAME" pin="AD2" pad="30"/>
<connect gate="&gt;NAME" pin="AD3" pad="32"/>
<connect gate="&gt;NAME" pin="AD4" pad="36"/>
<connect gate="&gt;NAME" pin="AD5" pad="37"/>
<connect gate="&gt;NAME" pin="AD6" pad="40"/>
<connect gate="&gt;NAME" pin="AD7" pad="41"/>
<connect gate="&gt;NAME" pin="AD8" pad="16"/>
<connect gate="&gt;NAME" pin="AD9" pad="15"/>
<connect gate="&gt;NAME" pin="ALEH" pad="35"/>
<connect gate="&gt;NAME" pin="ALEL" pad="33"/>
<connect gate="&gt;NAME" pin="CIC_DATA_CLK" pad="43"/>
<connect gate="&gt;NAME" pin="CIC_DATA_IO" pad="18"/>
<connect gate="&gt;NAME" pin="GND@1" pad="1"/>
<connect gate="&gt;NAME" pin="GND@2" pad="2"/>
<connect gate="&gt;NAME" pin="GND@22" pad="22"/>
<connect gate="&gt;NAME" pin="GND@23" pad="23"/>
<connect gate="&gt;NAME" pin="GND@25" pad="25"/>
<connect gate="&gt;NAME" pin="GND@26" pad="26"/>
<connect gate="&gt;NAME" pin="GND@27" pad="27"/>
<connect gate="&gt;NAME" pin="GND@31" pad="31"/>
<connect gate="&gt;NAME" pin="GND@47" pad="47"/>
<connect gate="&gt;NAME" pin="GND@48" pad="48"/>
<connect gate="&gt;NAME" pin="GND@50" pad="50"/>
<connect gate="&gt;NAME" pin="GND@6" pad="6"/>
<connect gate="&gt;NAME" pin="JTCK" pad="44"/>
<connect gate="&gt;NAME" pin="KEY@14" pad="14"/>
<connect gate="&gt;NAME" pin="KEY@39" pad="39"/>
<connect gate="&gt;NAME" pin="LAUDIO" pad="24"/>
<connect gate="&gt;NAME" pin="RAUDIO" pad="49"/>
<connect gate="&gt;NAME" pin="SI_CLK" pad="19"/>
<connect gate="&gt;NAME" pin="SI_DATA" pad="21"/>
<connect gate="&gt;NAME" pin="VIDEO_SYNC" pad="46"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICRO_USB" prefix="J">
<gates>
<gate name="G$1" symbol="MICRO_USB"/>
</gates>
<devices>
<device name="" package="MICRO_USB">
<connects>
<connect gate="G$1" pin="+5V" pad="1"/>
<connect gate="G$1" pin="DM" pad="2"/>
<connect gate="G$1" pin="DP" pad="3"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="GND1"/>
<connect gate="G$1" pin="GND@2" pad="GND2"/>
<connect gate="G$1" pin="GND@3" pad="GND3"/>
<connect gate="G$1" pin="GND@4" pad="GND4"/>
<connect gate="G$1" pin="GND@5" pad="GND5"/>
<connect gate="G$1" pin="GND@6" pad="GND6"/>
<connect gate="G$1" pin="ID" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MICRO_SD" prefix="J">
<gates>
<gate name="G$1" symbol="MICRO_SD"/>
</gates>
<devices>
<device name="" package="MICRO_SD">
<connects>
<connect gate="G$1" pin="CD1" pad="CD1"/>
<connect gate="G$1" pin="CD2" pad="CD2"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="CMD" pad="3"/>
<connect gate="G$1" pin="DAT0" pad="7"/>
<connect gate="G$1" pin="DAT1" pad="8"/>
<connect gate="G$1" pin="DAT2" pad="1"/>
<connect gate="G$1" pin="DAT3" pad="2"/>
<connect gate="G$1" pin="GND@6" pad="6"/>
<connect gate="G$1" pin="GND@G1" pad="G1"/>
<connect gate="G$1" pin="GND@G2" pad="G2"/>
<connect gate="G$1" pin="GND@G3" pad="G3"/>
<connect gate="G$1" pin="GND@G4" pad="G4"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="93C66" prefix="U">
<gates>
<gate name="G$1" symbol="93CX6"/>
</gates>
<devices>
<device name="" package="TSSOP8">
<connects>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DU" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="Q" pad="4"/>
<connect gate="G$1" pin="S" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATTINY45" prefix="U">
<gates>
<gate name="G$1" symbol="ATTINYX5"/>
</gates>
<devices>
<device name="" package="TSSOP8">
<connects>
<connect gate="G$1" pin="CLKI/PB3" pad="2"/>
<connect gate="G$1" pin="CLKO/PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="MISO/PB1" pad="6"/>
<connect gate="G$1" pin="MOSI/PB0" pad="5"/>
<connect gate="G$1" pin="RESET/PB5" pad="1"/>
<connect gate="G$1" pin="SCK/PB2" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W25Q128JVSIM" prefix="U">
<gates>
<gate name="G$1" symbol="SPI_MEMORY"/>
</gates>
<devices>
<device name="" package="SO8_208MIL">
<connects>
<connect gate="G$1" pin="/CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SIO0" pad="5"/>
<connect gate="G$1" pin="SIO1" pad="2"/>
<connect gate="G$1" pin="SIO2" pad="3"/>
<connect gate="G$1" pin="SIO3" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IS62WVS2568GBLL-45NLI" prefix="U">
<gates>
<gate name="G$1" symbol="SPI_MEMORY"/>
</gates>
<devices>
<device name="" package="SO8_150MIL">
<connects>
<connect gate="G$1" pin="/CS" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SIO0" pad="5"/>
<connect gate="G$1" pin="SIO1" pad="2"/>
<connect gate="G$1" pin="SIO2" pad="3"/>
<connect gate="G$1" pin="SIO3" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XLH336" prefix="X">
<gates>
<gate name="G$1" symbol="OSC"/>
</gates>
<devices>
<device name="" package="3.2X2.5_OSCILLATOR">
<connects>
<connect gate="G$1" pin="EN/NC" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="OUT2/NC" pad="5"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP7940N" prefix="U">
<gates>
<gate name="G$1" symbol="MCP7940N"/>
</gates>
<devices>
<device name="" package="TSSOP8">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="MFP" pad="7"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VBAT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FT2232HL" prefix="U">
<gates>
<gate name="G$1" symbol="FT2232H"/>
</gates>
<devices>
<device name="" package="LQFP64">
<connects>
<connect gate="G$1" pin="ACBUS0" pad="26"/>
<connect gate="G$1" pin="ACBUS1" pad="27"/>
<connect gate="G$1" pin="ACBUS2" pad="28"/>
<connect gate="G$1" pin="ACBUS3" pad="29"/>
<connect gate="G$1" pin="ACBUS4" pad="30"/>
<connect gate="G$1" pin="ACBUS5" pad="32"/>
<connect gate="G$1" pin="ACBUS6" pad="33"/>
<connect gate="G$1" pin="ACBUS7" pad="34"/>
<connect gate="G$1" pin="ADBUS0" pad="16"/>
<connect gate="G$1" pin="ADBUS1" pad="17"/>
<connect gate="G$1" pin="ADBUS2" pad="18"/>
<connect gate="G$1" pin="ADBUS3" pad="19"/>
<connect gate="G$1" pin="ADBUS4" pad="21"/>
<connect gate="G$1" pin="ADBUS5" pad="22"/>
<connect gate="G$1" pin="ADBUS6" pad="23"/>
<connect gate="G$1" pin="ADBUS7" pad="24"/>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="BCBUS0" pad="48"/>
<connect gate="G$1" pin="BCBUS1" pad="52"/>
<connect gate="G$1" pin="BCBUS2" pad="53"/>
<connect gate="G$1" pin="BCBUS3" pad="54"/>
<connect gate="G$1" pin="BCBUS4" pad="55"/>
<connect gate="G$1" pin="BCBUS5" pad="57"/>
<connect gate="G$1" pin="BCBUS6" pad="58"/>
<connect gate="G$1" pin="BCBUS7" pad="59"/>
<connect gate="G$1" pin="BDBUS0" pad="38"/>
<connect gate="G$1" pin="BDBUS1" pad="39"/>
<connect gate="G$1" pin="BDBUS2" pad="40"/>
<connect gate="G$1" pin="BDBUS3" pad="41"/>
<connect gate="G$1" pin="BDBUS4" pad="43"/>
<connect gate="G$1" pin="BDBUS5" pad="44"/>
<connect gate="G$1" pin="BDBUS6" pad="45"/>
<connect gate="G$1" pin="BDBUS7" pad="46"/>
<connect gate="G$1" pin="DM" pad="7"/>
<connect gate="G$1" pin="DP" pad="8"/>
<connect gate="G$1" pin="EECLK" pad="62"/>
<connect gate="G$1" pin="EECS" pad="63"/>
<connect gate="G$1" pin="EEDATA" pad="61"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@11" pad="11"/>
<connect gate="G$1" pin="GND@15" pad="15"/>
<connect gate="G$1" pin="GND@25" pad="25"/>
<connect gate="G$1" pin="GND@35" pad="35"/>
<connect gate="G$1" pin="GND@47" pad="47"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GND@51" pad="51"/>
<connect gate="G$1" pin="OSCI" pad="2"/>
<connect gate="G$1" pin="OSCO" pad="3"/>
<connect gate="G$1" pin="PWREN#" pad="60"/>
<connect gate="G$1" pin="REF" pad="6"/>
<connect gate="G$1" pin="RESET#" pad="14"/>
<connect gate="G$1" pin="SUSPEND#" pad="36"/>
<connect gate="G$1" pin="TEST" pad="13"/>
<connect gate="G$1" pin="VCCIO@20" pad="20"/>
<connect gate="G$1" pin="VCCIO@31" pad="31"/>
<connect gate="G$1" pin="VCCIO@42" pad="42"/>
<connect gate="G$1" pin="VCCIO@56" pad="56"/>
<connect gate="G$1" pin="VCORE@12" pad="12"/>
<connect gate="G$1" pin="VCORE@37" pad="37"/>
<connect gate="G$1" pin="VCORE@64" pad="64"/>
<connect gate="G$1" pin="VPHY" pad="4"/>
<connect gate="G$1" pin="VPLL" pad="9"/>
<connect gate="G$1" pin="VREGIN" pad="50"/>
<connect gate="G$1" pin="VREGOUT" pad="49"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="218-2">
<gates>
<gate name="G$1" symbol="SWITCH-2"/>
</gates>
<devices>
<device name="" package="218-2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
